

Central Registration Agent

User Requirements Specification

|  |  |
| --- | --- |
| Synopsis | This document describes the user requirements for the Central Registration Agent (CRA) system. |
| Version | 19.0 |
| Effective date |  |
| Prepared by | ELEXON Design Authority |

|  |
| --- |
| Intellectual Property Rights, Copyright and Disclaimer  The copyright and other intellectual property rights in this document are vested in ELEXON or appear with the consent of the copyright owner. These materials are made available for you for the purposes of your participation in the electricity industry. If you have an interest in the electricity industry, you may view, download, copy, distribute, modify, transmit, publish, sell or create derivative works (in whatever format) from this document or in other cases use for personal academic or other non-commercial purposes. All copyright and other proprietary notices contained in the document must be retained on any copy you make.  All other rights of the copyright owner not expressly dealt with above are reserved.  No representation, warranty or guarantee is made that the information in this document is accurate or complete. While care is taken in the collection and provision of this information, ELEXON Limited shall not be liable for any errors, omissions, misstatements or mistakes in any information or damages resulting from the use of this information or action taken in reliance on it. |

Table of Contents

[1 Management Summary 5](#_Toc529888977)

[2 Introduction 6](#_Toc529888978)

[2.1 Amendment History 7](#_Toc529888979)

[2.2 References 7](#_Toc529888980)

[2.3 Acronyms 7](#_Toc529888981)

[3 Scope of Specification 7](#_Toc529888982)

[4 Business and System Overview 9](#_Toc529888983)

[4.1 Summary of Business Requirements 9](#_Toc529888984)

[4.1.1 Registration Process 9](#_Toc529888985)

[4.2 Service Context 11](#_Toc529888986)

[4.3 User Requirements Source Documents 12](#_Toc529888987)

[4.4 Numbering Scheme for Requirement Definitions 12](#_Toc529888988)

[4.5 Attributes of Individual Requirements 13](#_Toc529888989)

[5 Functional Requirements 15](#_Toc529888990)

[5.1 CRA-F001: Register BSC Party 15](#_Toc529888991)

[5.2 CRA-F002: Maintain Authentication Data 17](#_Toc529888992)

[5.3 CRA-F003: Authenticate Party 18](#_Toc529888993)

[5.4 CRA-F004: Allocate BSC Party ID 18](#_Toc529888994)

[5.5 CRA-F005: Allocate BSC Party Energy Account 19](#_Toc529888995)

[5.6 CRA-F006: View / Maintain BSC Party Registration Details 19](#_Toc529888996)

[5.7 CRA-F007: Register Interconnector Administrator 21](#_Toc529888997)

[5.8 CRA-F008: View / Maintain Interconnector Administrator Data 22](#_Toc529888998)

[5.9 CRA-F009: Register BSC Party Agent 23](#_Toc529888999)

[5.10 CRA-F010: View / Maintain BSC Party Agent 25](#_Toc529889000)

[5.11 CRA-F011: Register BSC Service Agent 26](#_Toc529889001)

[5.12 CRA-F012: View / Maintain BSC Service Agent 27](#_Toc529889002)

[5.13 CRA-F013: BM Unit Registration 28](#_Toc529889003)

[5.14 CRA-F014: View / Maintain BM Unit Registration 31](#_Toc529889004)

[5.15 CRA-F015: Trading Unit Registration 35](#_Toc529889005)

[5.16 CRA-F016: View / Maintain Trading Unit Registration Details 36](#_Toc529889006)

[5.17 CRA-F017: Register CRA Boundary Points and System Connection Points Details 37](#_Toc529889007)

[5.18 CRA-F034: Register Metering System Details 39](#_Toc529889008)

[5.19 CRA-F018: View / Maintain Boundary Point and System Connection Point Details 41](#_Toc529889009)

[5.20 CRA-F019: View / Maintain Interconnector Registration 42](#_Toc529889010)

[5.21 CRA-F020: Maintain Credit Assessment Load Factor 43](#_Toc529889011)

[5.22 CRA-F021: Requirement not currently used 44](#_Toc529889012)

[5.23 CRA-F022: Issue Credit Assessment Capability 45](#_Toc529889013)

[5.24 CRA-F023: Validate Registrations 47](#_Toc529889014)

[5.25 CRA-F024: Report Registration Details 48](#_Toc529889015)

[5.26 CRA-F025: Distribute Register Data 49](#_Toc529889016)

[5.27 CRA-F026: Maintain Reference Data 50](#_Toc529889017)

[5.28 CRA-F027: SLA Reporting 51](#_Toc529889018)

[5.29 CRA-F028: Requirement not currently used 52](#_Toc529889019)

[5.30 CRA-F029: Register Interconnector 53](#_Toc529889020)

[5.31 CRA-F030: Register GSP Group and GSP Details 54](#_Toc529889021)

[5.32 CRA-F031: View / Maintain GSP Group Registrations 55](#_Toc529889022)

[5.33 CRA-F032: Maintain Transmission Loss Factors 56](#_Toc529889023)

[5.34 CRA-F033: Receive Registration Exception Reports 57](#_Toc529889024)

[5.35 CRA-F035: View / Maintain Metering System Details 58](#_Toc529889025)

[5.36 CRA-F036: Maintain Flexible Reporting Requirements 59](#_Toc529889026)

[5.37 CRA-F037: Transfer from SMRS 60](#_Toc529889027)

[5.38 CRA-F038: Transfer to SMRS 61](#_Toc529889028)

[5.39 CRA-F039: Register / View / Maintain Market Index Data Provider 62](#_Toc529889029)

[5.40 CRA-F040: Provide BSCCo with Withdrawals Checklist 63](#_Toc529889030)

[5.41 CRA-F041: GC and DC Breach Monitoring 64](#_Toc529889031)

[5.42 CRA-F042: Identify CRA-estimated GC and DC amounts 65](#_Toc529889032)

[5.42 CRA-F042: Identify CRA-estimated GC and DC amounts 66](#_Toc529889033)

[5.42 CRA-F043: Manage GC and DC Breach Challenges 67](#_Toc529889034)

[6 Interface Requirements 68](#_Toc529889035)

[7 Non Functional Requirements 73](#_Toc529889036)

[7.1 CRA-N001: Input Interface Requirements 73](#_Toc529889037)

[8 Service Requirements 75](#_Toc529889038)

[8.1 CRA-S001: Message Security and Encryption 75](#_Toc529889039)

[8.2 CRA-S002: Data Migration Requirements 75](#_Toc529889040)

[8.3 CRA-S003: Archiving Requirements 76](#_Toc529889041)

[9 User Roles and Activities 77](#_Toc529889042)

[10 Future enhancements 78](#_Toc529889043)

[Appendix A Requirements Compliance Matrix 79](#_Toc529889044)

[Appendix B Logical Data Model 82](#_Toc529889045)

[Appendix C Business Process Model 83](#_Toc529889046)

[Appendix D NETA Central Service Common Non Functional Requirements 84](#_Toc529889047)

[Appendix E NETA Central Services Common Service Requirements 89](#_Toc529889048)

[Appendix F NETA Central Services Common Future Requirements 95](#_Toc529889049)

[Appendix G Glossary 96](#_Toc529889050)

# 1 Management Summary

The Central Registration Agent (CRA) is one of the suite of seven services that support the operation of the Balancing and Settlement Code (BSC).

The role of the CRA is to maintain a master register of information relating to the registration of participants, trading units and physical plant such as Boundary Points and interconnectors. The principal business processes involved may be summarised as:

* The registration and Qualification of BSC Parties;
* The registration and maintenance of BM Unit and Trading Unit details received from the BSC Party as well as Credit Assessment details from the Settlement Administration Agent (SAA);
* The registration of CRA Boundary Points, System Connection Points and Metering Systems received from the BSC Party;
* The reception and maintenance of requests for Agent Qualification; together with a list of Agents who have passed all Qualification processes and can support BSC Parties obligations.
* The validation and correlation of these individual Registration instructions to ensure accuracy, completeness and consistency within the system;
* The distribution of Registration reports to the BSC Parties on the occurrence of processing of requests and registration information;
* The distribution of Registration details to other components of the BSC central system services either on demand or as batch processing;
* The monitoring of BM Units’ Metered Volumes to identify GC or DC breaches (GC and DC Breach Monitoring) and the subsequent estimation of BM Unit Metered Volumes (CRA-Estimated GC or DC Amounts) to update BM Units GC or DC

The purpose of this document is to provide a complete specification of the set of business requirements that the CRA Service must satisfy for all of its various User types. These range from the BSC Parties, to BSCCo Ltd and its various Agents, including the operators of the CRA itself and the other BSC Services. Similar documents define the requirements for the other Services.

A convention has therefore been used for uniquely identifying the requirements in each document. This ensures that the fulfilment of each requirement can be unambiguously traced through the subsequent functional specification, design and implementation. This is of particular importance for the implementation of the SAA, CRA and CDCA services, which will use a single integrated computer system. This document does not, however, attempt to describe the integration of those services, which would be inappropriate for this CRA User Requirement Specification (URS).

The requirements that have been identified have been divided into four categories:

* Functional (F), a specific business requirement of the service.
* Non-functional (N), which includes auditing, security, resilience etc. The majority of these will probably be associated with the General (GEN) service.
* Service (S), which includes all time-related service delivery requirements, including performance and volumetrics.
* Interface (I), a requirement for data exchange between services or to / from external parties.

These requirements are catalogued in sections 5 to 8 respectively with the common requirements placed in appendices of this document

# 2 Introduction

This document is the User Requirements Specification (URS) for the Central Registration Agent role within the Balancing and Settlement Code Services. It is one of a set of documents forming the baseline for requirements of seven BSC central system services. This document set comprises (but does not exclude further Services):

* BMRA URS;
* CRA URS;
* SAA URS;
* TAA URS;
* ECVAA URS;
* CDCA URS;
* FAA URS;
* Interface Definition and Design (IDD).

The objective of this document is to provide a complete specification of the requirements that the CRA Service must meet, from the users’ point of view. For this purpose, the “users” include BSCCo Ltd, Ofgem, National Grid as the Balancing Mechanism Operator, other Service Providers, BSC Parties, and the CRA Service Provider’s own user Operators.

Note that the current solution for the BSC central systems involves a bundled approach where the requirements of the SAA, CRA and CDCA Services are met within the same computer system. As this URS is describing the requirements of the CRA *service* in isolation, this document does not attempt to identify in detail where common requirements of these Services will be met by a shared function in the solution.

Note that, subsequent to the introduction of P62, any of the following terms can represent a Licensed Distribution System Operator (LDSO) or any Party which distributes electricity.

* Distribution Business
* Distribution System Operator
* Public Distribution System Operator (and abbreviation PDSO)
* Distribution Company
* Public Electricity Suppliers (PES), as operators of a distribution network
* Distributor, as operator of a distribution network

This document refers to a “Supplier BM Unit”, which means a BM Unit with a BM Unit Type of ‘G’ or ‘S’, as stated by the Lead Party on the ‘Registration of BM Unit’ form in BSCP15.

## 2.1 Amendment History

| Date | Issue | Description of Change | Reference |
| --- | --- | --- | --- |
| 28/01/10 | 15.0 | Issued |  |
| 23/02/12 | 16.0 | Document rebadged and amended for February 2012 Release (P268 & P269) | ISG130/08 |
| 25/06/15 | 17.0 | Modification P310; June 2015 Release | ISG169/05 |
| 23/02/17 | 18.0 | CP1471 | ISG185/03 |
|  |  | P326 Self-Governance | ISG188/05, ISG191/01 |
| 29/06/17 | 19.0 | P350 for the June 17 Release | ISG194/02 |

Further details of this document’s amendment history are available from BSCCo on request.

## 2.2 References

|  |  |
| --- | --- |
| CRA SD | Service Description for Central Registration Agent (NETA Programme) |
| TAA SD | Service Description for Technical Assurance Agent (NETA Programme) |
| CDCA SD | Service Description for Central Data Collection Agent (NETA Programme) |
| SAA SD | Service Description for Settlement Agent (NETA Programme) |
| CRA BPM | RETA Business Process Models [CRA] - (NETA Programme) |
| NETA SCH | NETA Service Agreement (NETA Programme) |
| CRAWS | CRA Workshop held on 01/02/2000 |
| DID-2 | Data Items Definition Design Clarification version 2 (NETA Programme) 17/02/2000 |
| PPR | Program Progress Report (01/03/2000) |
| IDD | Interface Definition and Design (Parts 1 & 2) |

## 2.3 Acronyms

See Appendix for the full glossary of terms.

# 3 Scope of Specification

This document provides a complete specification of the requirements for the Central Registration Agent (CRA) Service within the NETA programme. The requirements are described from the point of view of the CRA Service Users.

The document is divided into the following chapters.

* Chapter 4, Business and System Overview - describes the business context of the CRA Service. It includes a definition of the CRA Service User population.
* Chapter 5, Description of Requirements - describes the functional requirements of the Service from the point of view of the Service users.
* Chapter 6, External Interfaces - describes the interfaces with the external users of the Service.
* Chapter 7, Non Functional Requirements - describes the non-functional requirements of the Service.
* Chapter 8, Service Requirements - describes the service requirements for the Service.
* Chapter 9, User Roles and Activities - describes the users of the system and their interaction with the CRA.
* Chapter 10, Future Enhancements - describes potential functional enhancements.
* Appendix A - presents a Requirements Compliance Matrix against the CRA Service Description documentation.
* Appendix B - presents the Logical data model as it relates to the CRA system.
* Appendix C presents the provided Business Process Model
* Appendix D presents the Common User Requirements for the Non Functional Requirements.
* Appendix E presents the Common User Requirements for the Service Requirements.
* Appendix F presents the Common Future Requirements for the Service Requirements.
* Appendix G presents the Glossary of Terminology used within the whole BSC Central Systems Specifications[[1]](#footnote-2).
* This format is as specified in section 5 of our proposal.

# 4 Business and System Overview

This section provides an overview of the business and systems involved within the CRA system. The overview is for indicative purposes only. Section 5 and the requirements detailed therein form the definitive statement of requirements.

## 4.1 Summary of Business Requirements

The role of the CRA is to maintain a master register of information relating to the registration of participants, trading units and physical plant such as Boundary Points and interconnectors. The principal business processes involved may be summarised as:

* The registration and Qualification of BSC Parties;
* The registration and maintenance of BM Unit and Trading Unit details received from the BSC Party as well as Credit Assessment details from the Settlement Administration Agent (SAA);
* The registration of CRA Boundary Points, System Connection Points and Metering Systems received from the BSC Party;
* The reception and maintenance of requests for agent Qualification; together with a list of agents who have passed all Qualification processes and can support BSC Parties obligations.
* The validation and correlation of these individual Registration instructions to ensure accuracy, completeness and consistency within the system;
* The Generation Capacity (GC) / Demand Capacity (DC) breach monitoring and resultant adjustment of GC and/or DC values;
* The distribution of Registration reports to the BSC Parties on the occurrence of processing of requests and registration information;
* The distribution of registration details to other components of the NETA system either on demand or as batch processing.

### 4.1.1 Registration Process

With the exception of functionality concerning the calculation of credit assessment import and export capabilities, the bulk of the CRA functionality is to log, store and forward registration information. The CRA shall receive this information for a variety of object types, but the manner in which they are entered into the system is common across types.

Registration requests are sent to the CRA in either manual (paper based, e-mail) or electronic format from the relevant Party. An Operator (for definition of this term see Section 9) shall then be able to enter the details into the appropriate registration form, correlate that any supporting documentation has been received, and save the data.

Where the input data has been sent to the CRA through an automated electronic flow, the system shall present the Operator with a human readable version of the data from which the data may be “cut and pasted” from one screen to another.

Where the data has been sent to the CRA through a manual mechanism, the Operator shall enter the details from the original medium into the CRA.

This process, regardless of registration object, thus has a number of key, common features. These are detailed in CRA-N001 and summarised below prior to the individual functional requirements.

1. All registration actions or changes to registered data shall require the prior approval of BSCCo Ltd. This is expected to be in the form of paper based supporting documentation. An Operator shall be expected to check that this authorisation has been received when processing the Registration request and facilities (tick-boxes, document reference fields) will be available on the input forms to

 allow for cross-referencing between paper and electronic registration information;

 log that this check has been completed

2. Should the data, once entered on the input form fail input validation, the Operator will be presented with the failure reason. The Operator shall then be presented with the ability to save the valid parts of the registration (subject to database constraints) in a “Pending” state rather than having to abort the entire update. While in this state, the data will be “invisible” to other parts of the BSC Central Systems. For instance it will not be issued to other Services (CDCA, SAA). At a later time, the Operator shall be able to retrieve the partial update and complete the registration operation when the original failure has been corrected.

3. Certain registration items (such as BM Units) are expected to be registered from a limited sub-set of Party types. The CRA system shall ensure that a check against Party type is conducted on entry or amendment of registration details. However, where an unexpected registration request is detected, the CRA shall not fail the operation outright. Rather, the Operator shall be required to override the warning explicitly.

4. When overriding a “Warning” from either point 2 and 3 above, it may be necessary that the level of authority for the override operation be increased from an Operator. A Supervisor may, in some cases, be required to clear a specific Warning type. These roles shall be described in more detail in the CRA System Specification.

5. All registration entries / amendments shall be tagged with the date and time of the operation as well as the identifier (username) of the Operator who entered the details. In addition, where a validation Warning is expressly overridden, the Operator / Supervisor’s identification will also be logged.

6. Each registration operation may require a specific level of authorisation within the requesting Party. The CRA stores these levels of authorisation and shall validate that the requesting person has the authorisation to conduct the requested operation. Where this check fails the CRA shall reject the entire request.

7. The CRA system shall (with exceptions such as on change of ownership of BM Units and Interconnector Error Administration responsibility) only accept registration amendments from the Party that sent in the original registration request.

## 8. Where data is to be input manually, the service shall use reasonable endeavours to ensure that the quality of the data is not compromised in any way.4.2 Service Context

The following diagram illustrates the context of the CRA service within the wider market of the Balancing and Settlement Code. This is a simplified view for clarity; section 6 describes the interfaces from the CRA service to other Parties in detail.

BMRA

CRA

SAA

TAA

ECVAA

CDCA

FAA

BSC Party

SO

SVAA

IA

BSCCo

IEA

Public

MIDP

MVRNA

ECVNA

Meter

MOA

BSC Party

Credit Agency

Bank

| Item | Description |
| --- | --- |
|  |  |
| Bank | A bank that receives debit and credit instructions from the Funds Administration Agent. |
| BMRA | Balancing Mechanism Reporting Agent. |
| BSC Party | Any user of Balancing and Settlement Code services. |
| BSCCo Ltd | The Balancing and Settlement Code Company. |
| CDCA | Central Data Collection Agent. |
| CRA | Central Registration Agent |
| Credit Agency | A credit agency that provides credit cover data on Parties. |
| ECVAA | Energy Contract Volume Aggregation Agent. |
| ECVNA | Energy Contract Volume Notification Agent. |
| FAA | Funds Administration Agent. |
| IA | Interconnector Administrator. |
| IEA | Interconnector Error Administrator |
| Meter | A physical meter registered within the Balancing and Settlement Code arrangements. |
| MIDP | Market Index Data Provider |
| MOA | Meter Operation Agent. |
| MVRNA | Metered Volume Reallocation Notifications Agent |
| Public | A member of the general public. |
| SAA | Settlement Administration Agent. |
| SO | System Operator |
| SVAA | Supplier Volume Aggregation Agent |
| TAA | Technical Assurance Agent. |
|  |  |
| Transfer Coordinator | A role undertaken by BSCCo Ltd to coordinate transfers of metering between CVA (CRA & CDCA) and SVA in order to address the risk that Metering Systems are ‘double counted’ or ‘omitted’ from Settlements’. |

## 4.3 User Requirements Source Documents

In addition to our tender, the reference documents listed in section 1.5 have been used. The code listed in the first column is used as a cross reference in the detailed requirement specifications listed in section 5.

## 4.4 Numbering Scheme for Requirement Definitions

The present solution maps the requirements for the BSC Services across a number of computer systems plus a set of manual processes, so it is vital that each requirement across the set of services is uniquely identified. This allows us to trace through each individual requirement from URS to System Specification (i.e. functional specification) and then to Design Specification (technical specification).

In keeping with industry good practice, this URS adopts a requirements numbering system that works as follows:

1. Each requirement is associated with either an individual service, or is common to all services supported by our systems (i.e. TAA will typically be excluded from the latter). If a requirement applies to more than one service, but not all (e.g. two out of six), then the requirement is restated for each, i.e. there would be two separately numbered requirements (which happen to be the same) in this example.

Each requirement is prefaced by one of the following codes, as a clear indicator as to which service generates the business need:

* CRA (Central Registration Agent);
* SAA (Settlement Administration Agent);
* CDCA (Central Data Collection Agent);
* ECVAA (Energy Contract Volume Aggregation Agent);
* BMRA (Balancing Mechanism Reporting Agent);
* TAA (Technical Assurance Agent);
* FAA (Funds Administration Agent);
* GEN (General).

2. Requirements are categorised into the following headings:

* Functional (F), a specific business requirement of the service.
* Non-functional (N), which includes auditing, security, resilience, etc.
* Service (S), which includes all time-related service delivery requirements, including performance and volumetrics.
* Interface (I), a requirement for data exchange between services or to and from external parties.

3. Within a service, each requirement has a unique number in the range 001 to 999. Numbers are not unique across services. Leading zeroes are always included.

Combining 1, 2 and 3 thus gives the following format for numbering each requirement (including a separator character):

***[Service]-[Category][Number]***

For example:

 CRA-F001

 BMRA-S022

 GEN-N112

 SAA-I033

## 4.5 Attributes of Individual Requirements

For each identified requirement, the following items of information are represented in a tabular format:

**Requirement ID:** A unique identifier for the requirement, as described above.

**Status:** While the majority of CRA requirements will be mandatory for the Go Live date, others may not necessarily be. This field indicates whether the requirement is Mandatory (M) or Optional (O) in this context.

**Title:** A short descriptive title for the requirement.

**BSC reference:** A cross reference to the BSC section which is the original source of the business need. Note that there may be detailed requirements identified in the User Requirements Specification which are not individually described in the BSC; in this case this field is used to reference the alternative source of the requirement, for instance a specific workshop with the customer’s user community. The references shall use the abbreviations in section 1.5 above.

**Man/Auto:** This field provides an indication as to whether a given requirement is likely to be satisfied by a manual, as opposed to automated, mechanism. This is not however intended to be prescriptive, and the approach to supporting any individual requirement will be made definitively during the design phase.

**Frequency:** An indication of how often a business event will take place. Minimum, maximum and average frequencies, and any timing or scheduling requirements, are also identified here, as appropriate.

**Volumes:** Data volumes associated with the requirement are identified here; this may include an estimate of the initial volume, and subsequent growth rates.

The requirement is then described in detail, with any associated specific non-functional and interface requirements separately identified.

# 5 Functional Requirements

This section describes the detailed set of business requirements for the Central Registration Service. To ensure traceability through to other deliverable documents such as the System Specification and Design Specification, each requirement is assigned a unique number, based on the convention described in section 4. The requirements have been constructed, at this version of the document from the documents referenced as in chapter 1.

## 5.1 CRA-F001: Register BSC Party

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F001 | **Status:**  Mandatory | **Title:**  Register BSC Party | **BSC Reference:**  CRA SD 4.1, CRA SD 4.2, CRA SD 4.3, CRABPM 3.1, CRAWS -20, CR\_18\_990909, P197 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Mostly at initial set-up | |
| **Functional Requirement:** | | | |
| The CRA shall allow an Operator to manually enter new BSC Party Registration Information into the CRA system.  The CRA system shall recognise a set of BSC Party types including (and not exclusively):  a) Transmission Owner,  b) System Operator,  c) Distribution Company,  d) Interconnector Administrator,  e) Trading Party  f) Interconnector Error Administrator (Note: These will be associated with pseudo-BM Units and will have Energy Accounts)  In addition, Trading Parties may have one or more of the following roles:  i) Generator  ii) Supplier  iii) Trader (Non Physical)  iv) Interconnector User  Each of the Party types and roles allow for a different set of registration requests to be processed by the system. (For instance a non-physical Trader should not in the main be allowed to register Interconnectors). Where an attempt is made and is not expected according to role, the CRA shall flag a Warning as specified in CRA-N001. The following table illustrates these relationships.    These registration requests shall subsequently be received by the CRA in accordance with the other requirements in this specification. None of these later requests shall be processed until the initial BSC Party Registration has been completed.  The BSC Party shall submit registration information to the CRA system including details of:   An Action Description to specify the type of registration operation,   the Party (name, contact details),   the Party’s Stage 2 Names (where they exist).   authorised signatories and individual contact details,   settlement report distribution requirements,   Party Agents that the Party shall use,  A detailed description of the interface content may be found in CRA-I001.  Along with the details of the registration request from the BSC Party, the CRA shall receive supporting information from BSCCo Ltd. BSC Parties shall not be able to complete registration with the CRA before they have completed Qualification Processes. CRA will receive authorisation from BSCCo Ltd to register a particular party.  The input data shall be validated in accordance with the following rules:  1) The Party Types associated with the BSC Party Registration are valid according to the valid set of Party type standing data,  2) Each Interconnector that is used by the BSC Party conforms to a valid Interconnector ID stored within the system.  3) Where a BSC Party states a change to the usage of an Interconnector, that these details match those received from the Interconnector Administrator (both in usage type and effective to and from dates).  4) That where the BSC Party is the Interconnector Error Administrator for an Interconnector, the details match those received from the Interconnector Administrator registration details (both in responsibility and effective to and from dates).  5) That the Party Agents that the Party shall use are registered for the period of the registration request.  6) That there is at least one authorised signatory sent to the CRA.  Where the data has passed validation the information shall be stored within the CRA system database after being authorised by a Supervisor. Any authentication details (authorised signatories) referenced within the message shall be stored according to the requirements of CRA-F002. The CRA system shall then allocate and return to the Operator a meaningful and unique BSC Party ID and two energy account identifiers (derived from the BSC Party ID) in accordance with CRA-F004 and CRA-F005.  The CRA system shall also provide the BSC Party with sufficient information for the authentication of future communications, electronic or otherwise.  Where the BSC Party is of a type “Supplier” the CRA system shall trigger the registration of one BM Unit registration request for each GSP group in accordance with the requirements of CRA-F013. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input interfaces:  CRA-I001  Output Interfaces:  CRA-I014  CRA-I015  CRA-I013  CRA-I012 | | | |

## 5.2 CRA-F002: Maintain Authentication Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F002 | **Status:**  Mandatory | **Title:**  Maintain Authentication Data | **BSC Reference:**  CRA BPM 3.1, CRA SD 4.2.2, CRA SD 4.1.7, CRAWS-21, CP756 CP1193 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low, a few 10’s per month after initial set-up. | |
| **Functional Requirement:** | | | |
| The CRA shall allow an Operator to enter and maintain authentication data against which incoming BSC party registration requests may be authenticated. The CRA will also obtain and maintain authentication information from BSCCo Ltd nominated signatories.  The authentication details (authorised signatory, password and optionally an e-mail address) will be stored within the system against the BSC Party along with the authentication key for the BSC Party.  Where the password for an authorised signatory is changed, the old password must be entered correctly in order for the update to take place. Only if the current password is entered correctly will the new password be accepted. The new password will then be effective for all authentication processes from the date and time at which the update was accepted.  In the special case where a BSC Party has no current authorised signatories, the first entrant shall be accepted without confirmation checks. Validation that this signatory’s name and password is correct shall be a manual process according to CRA-F001.  The new authentication details shall be distributed to the BSCCO, FAA, ECVAA and SAA systems according to the distribute register data requirement (CRA-I013) by 5.00pm on the day of update or additionally as necessary. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Output Interfaces:  CRA-I013 | | | |

## 

## 5.3 CRA-F003: Authenticate Party

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F003 | **Status:**  Mandatory | **Title:**  Authenticate Party | **BSC Reference:**  CRA BPM 3.1, CRA SD 4.1, CP756 |
| **Man/Auto:**  Automatic/ Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall perform authentication validation between authentication data contained on incoming registration requests against that held within the system. The system authentication data will have been entered previously through process CRA-F002.  The authentication check shall consist of validating the password of the authorised signatory against that held within the system.  Where the request is received via e-mail, the authentication check will validate the password and the sender’s e-mail address against those held within the system for the authorised signatory. A request received via e-mail can only be authenticated if the signatory has a registered password.  The success / failure of all authentication checks will be maintained within the system along with the date and time of the request. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.4 CRA-F004: Allocate BSC Party ID

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F004 | **Status:**  Mandatory | **Title:**  Allocate BSC Party ID | **BSC Reference:**  CRA BPM 3.1, CRA SD 4.1.2, CRAWS-24 |
| **Man/Auto:**  Automatic | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall, on receipt of a new BSC Party Registration request, create a unique and meaningful party identifier irrespective of role.  The CRA system shall perform a check against the name of the BSC Party and currently stored BSC Parties.  To avoid errors of duplication, should a potential duplicate BSC Party name be found, the system will issue a warning which must be overridden prior to allocation of a new identifier. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.5 CRA-F005: Allocate BSC Party Energy Account

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F005 | **Status:**  Mandatory | **Title:**  Allocate BSC Party Energy Account | **BSC Reference:**  CRA BPM 3.1, CRA SD 4.1.2, CRAWS-25 |
| **Man/Auto:**  Automatic | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall, on request, allocate energy account identifiers for a BSC Party. Two energy accounts must be allocated to any individual BSC Party (one for production, one for consumption). A standard convention will be used for identification of the account based upon the BSC Party Identifier. The effective start date of the energy account shall be provided to the CRA system and stored against the accounts. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.6 CRA-F006: View / Maintain BSC Party Registration Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F006 | **Status:**  Mandatory | **Title:**  View / Maintain BSC Party Registration Details | **BSC Reference:**  CRA BPM 3.1, CRA SD 4.1.1, CRAWS-20, CRAWS-26, CP508 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low, expected rate to be a few 10’s per month. | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator of the system to view and amend the details of a BSC Party. The CRA shall allow a BSC Party to change any part of its registration information as specified in CRA-I001 and CRA-F001.  In addition, the system shall provide functionality for the de-registering of a BSC Party in accordance with the specific functionality detailed in the deregistration requirement below:  The system shall validate the authentication details (signatory and password) contained within the message against those held currently against the BSC Party in accordance with requirement CRA-F004.  The input data shall be validated in accordance with the following rules:  1) Any change to the Party Types associated with the BSC Party Registration are valid according to the valid set of Party type standing data,  2) Any Interconnector usage specified by the BSC Party references a valid Interconnector ID stored within the system.  3) Where a BSC Party states a change to the usage of an Interconnector. that these details match those received from the Interconnector Administrator (both in usage type and effective to and from dates).  Changes, addition or amendment to authorisation data, shall be handled according to the requirements in CRA-F002.  Viewing of certain information, such as the authentication details for the Party, may be restricted to authorised personnel only.  BSC Party information may not be physically deleted from the system, it may only be logically deleted.  Registration changes relating to participant capacity or authorised person shall be confirmed by BSCCo Ltd in order to ensure that the new registration details are valid and are consistent with the current status of the BSC Party. This confirmation shall be submitted via a CRA-I001 flow from BSCCo Ltd containing the change. The registration changes requiring this confirmation are:   Add new party role   Change party role effective dates   Change Stage 2 participant details   Add, remove authorised signatory   Add authorisation level   Change effective dates on authorisation level   Changes Interconnector Administration details  Other registration changes do not require confirmation by BSCCo Ltd. | | | |
| **Deregistration of BSC Party**  In the special case where a BSC Party is de-registered, the CRA system shall check the validity of the termination request by ensuring that all sub-ordinate registrations for the Party (such as BM Units) have been de-registered prior to the request. Where this has not occurred, the CRA system shall inform the Operator of the fact and await confirmation of action.  The CRA shall require the explicit prior approval of the deregistration from BSCCo Ltd. | | | |
| **Non Functional Requirement:** | | | |
| If the Party sends a “CRA-I001 Receive BSC Party Registration Data” flow to CRA which requires authorisation by BSCCo Ltd as described above, then CRA will forward this directly to BSCCo Ltd. (Note: once the data has been forwarded to BSCCo Ltd, the flow processing has been completed. If BSCCo Ltd approve the change then BSCCo Ltd will submit a CRA-I001 to CRA containing the approved changes.) | | | |
| **Interfaces:** | | | |
| Input interfaces:  CRA-I001  Output Interfaces triggered from this action:  CRA-I014  CRA-I015  CRA-I013  CRA-I028 | | | |

## 5.7 CRA-F007: Register Interconnector Administrator

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F007 | **Status:**  Mandatory | **Title:**  Register Interconnector Administrator | **BSC Reference:**  CRA SD 4.1.3, CRAWS-20, CRAWS-27, CRAWS-28 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall allow an Operator to enter registration details for an Interconnector Administrator. The details shall consist of:   An Action Description   Interconnector Administrator Identification and Authentication Data   Contact Details   Interconnector Details   Interconnector Error Administrator Details  A detailed description may be found in the requirements for CRA-I002.  The CRA system shall validate incoming data according to the following rules:  1) That each of the Interconnectors specified in the details are registered within the system,  2) That no other Interconnector Administrator is assigned to the Interconnector.  Where an Interconnector Administrator is already specified for the Interconnector, the system shall only allow the request to proceed if the effective from date of the new Interconnector Administrator matches the effective to date of the currently stored record.  Where data is registered in respect of an Interconnector Error Administrator, the CRA shall require the explicit authorisation of BSCCo Ltd.  The CRA system shall accept registration requests as per CRA-I002 where no Interconnector Error Administrator is specified on initial registration. This condition will be reported to the Operator for confirmation on entry and subsequently reported in accordance with the requirements of CRA-F023. Assignment of an Interconnector Error Administrator may then be conducted at a later time through CRA-F008. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I002  Output Interfaces triggered from this action:  CRA-I014  CRA-I015  CRA-I019  CRA-I020 | | | |

## 5.8 CRA-F008: View / Maintain Interconnector Administrator Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F008 | **Status:**  Mandatory | **Title:**  View / Maintain Interconnector Administrator Data | **BSC Reference:**  CRA SD 4.1.3, CRAWS-29 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to view / amend the details of an Interconnector Administrator registration.  The CRA system shall allow the Interconnector Administrator to change any details of the registration. The CRA will be sent any changes, including:   An Action Description   Interconnector Administrator Identification and Authentication Data   Contact Details   Interconnector Details   Interconnector Error Administrator Details  A detailed description can be found in the requirements for CRA-I002.  Where the details state that the Interconnector Administrator is ceasing registration of the role, it is the responsibility of the Operator to ensure that this obligation has the agreement of BSCCo Ltd. This shall be conducted by review of supporting documentation from BSCCo Ltd and the fact that this check has been conducted shall be enterable against the transaction. The system shall then prompt the Operator to register the new Interconnector Administrator (through CRA-F007). If this cannot be entered, the fact that the Interconnector has no Administrator shall be flagged through CRA-F023 daily while this situation persists.  Where data is sent concerning a change of Interconnector Error Administrator, the data provided from the Interconnector Administrator shall require the explicit authorisation of BSCCo Ltd. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.9 CRA-F009: Register BSC Party Agent

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F009 | **Status:**  Mandatory | **Title:**  Register BSC Party Agent | **BSC Reference:**  CRA SD 4.2, CRA SD 5, CRA BPM 3.5, CRAWS-30, P197 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low, Few 10’s per month | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to enter the registration details for a BSC Party Agent.  The range of valid BSC Party Agent types shall be defined as (not exclusively):  a) Energy Contract Volume Notification Agents,  b) Metered Volume Reallocation Notification Agents  c) Half Hourly Data Collector Agents  d) Half Hourly Data Aggregator Agents  e) Half Hourly Meter Operator Agents  f) Non Half Hourly Data Collector Agents  g) Non Half Hourly Data Aggregator Agents  h) Non Half Hourly Meter Operator Agents  i) Meter Administration Agent  j) Supplier Meter Administration Agent  The CRA shall receive the following information from BSCCo Ltd:   Authentication Details   BSC Party Agent Details   Individual Authorisation Details and signatories   Certification /Accreditation Details[[2]](#footnote-3)  Full details of the flow may be found in CRA-I003.  It is expected that the initial Registration from BSCCo Ltd may consist of only the BSC Party Agent Details and Qualification Details. The remainder of the registration details (such as Authorised Signatories) would be sent later by either the BSC Party Agent or BSCCo Ltd.  It shall be the responsibility of an operator of the CRA system to validate the following data against paper documentation:  1) That the BSC Party Agent has been registered with BSCCo Ltd,  2) That the BSC Party Agent has been Qualified.  Confirmation that each of these checks has been conducted shall be enterable into the CRA system alongside the entering Operator’s identification details.  The system shall store the authentication data contained in the flow according to the requirements of CRA-F002.  The CRA shall only accept a registration where the BSC Party Agent has a valid Qualification status (where applicable). Where the Qualification status is not valid, the details may be entered into the system though the BSC Party Agent will not be regarded as Registered. The Qualification status may subsequently be amended through the View / Maintain BSC Party Agent Registration requirement, at which point the Registration of the Agent will be completed.  On successful registration of the BSC Party Agent, a report detailing the BSC Party Agent, Registration, and Qualification Details shall be triggered. (CRA-I024) | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I003  Output interfaces:  CRA-I013  CRA-I014  CRA-I024 | | | |

## 5.10 CRA-F010: View / Maintain BSC Party Agent

| **Requirement ID:**  CRA-F010 | **Status:**  Mandatory | **Title:**  View / Maintain BSC Party Agent | **BSC Reference:**  CRA SD 4.2, CRAWS-30, CP503, P197 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low, Few 10’s per month | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to view and maintain BSC Party Agent details.  The BSC Party Agent Registration amendment will concern elements of the following data:   Authentication Details   BSC Party Agent Details   Individual Authorisation Details and signatories   Certification/Accreditation Details[[3]](#footnote-4)  Full details of the flow may be found in CRA-I003.  The system shall validate that:  1) In the case where the amendment is to de-register an ECVNA or MVRNA, that the agent has no authorisations registered with ECVAA beyond the agent termination date. This communication is described by the requirements CRA-I036 and CRA-I037.  The system shall allow for the amendment of the Qualification and registration details as well as the details concerning the BSC Party Agent itself (such as address and contact data).  The CRA shall provide a mechanism for the management and storage of re-Qualification data where re-Qualification becomes necessary.  Where the registration update is to de-register a BSC Party Agent, the system shall inform all BSC Parties that have specified a use of the Agent. Affected Parties will continue to be flagged in the CRA system through CRA-F023. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I003  Output interfaces triggered from this activity:  CRA-I013  CRA-I014  CRA-I024  ECVAA Validation interfaces:  CRA-I036  CRA-I037 | | | |

## 5.11 CRA-F011: Register BSC Service Agent

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F011 | **Status:**  Mandatory | **Title:**  Register BSC Service Agent | **BSC Reference:**  CRA SD 4.3, CRAWS-31, P82, P197 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to enter the registration details for the following BSC Service Agents, operating under the direct control of BSCCo Ltd. The list shall include:  1) Supplier Technical Assurance Agent  2) Supplier Teleswitch Support Agent  3) Supplier Volume Aggregation Agent  4) Settlement Administration Agent  5) Balancing Mechanism Reporting Agent  6) Energy Contract Volume Aggregation Agent  7) Funds Administration Agent  8) Supplier Volume Allocation Agent  9) Central Data Collection Agent  10) Central Registration Agent  The following information concerning the Service Agent is supplied by BSCCo Ltd:   Name   Type   Contact Details  Full details of the interface may be found in CRA-I004.  The system shall validate that:  1) The name entered against the Service Agent is not already contained within the database. Should a duplicate name be found, the system shall issue a warning and ask the Operator for confirmation prior to acceptance.  2) The Agent Type is compliant with one of the agent types described above.  It shall be the responsibility of an Operator of the CRA system to validate the following data against paper documentation:   That the BSC Service Agent has been registered with BSCCo Ltd | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CR-I004  Output Interfaces triggered by this activity:  CR-I013  CR-I014  CR-I021 | | | |

## 5.12 CRA-F012: View / Maintain BSC Service Agent

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F012 | **Status:**  Optional | **Title:**  View / Maintain BSC Service Agent | **BSC Reference:**  CRA SD 4.3, CRAWS-31 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to view and maintain BSC Service Agent details.  The following information is presented from BSCCo Ltd concerning the Service Agent:   Name   Type   Contact Details  Any change to the BSC Service Agent details that results in a change of the registration state shall trigger the production of a registration report. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CR-I004  Output Interfaces triggered by this activity:  CR-I013  CR-I014  CR-I020  CR-I021 | | | |

## 5.13 CRA-F013: BM Unit Registration

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F013 | **Status:**  Mandatory | **Title:**  BM Unit Registration | **BSC Reference:**  CRA SD 6.1, CRA BPM 3.2, NGC VAL 3.0, CRAWS-32, DID-2, CP753, CP775, P100, P215, P268, P269 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to enter details of a BM Unit registration into the system. BM Units may be of 5 6 principal (though not exclusively limited to these) types:  i) Directly Connected BM Unit  ii) Supplier BM Unit  iii) Embedded site within GSP Group  iv) Interconnector Error Administrator BM Unit  v) Interconnector User BM Unit  Only Trading Parties should in the main be allowed to register BM Units though other Parties shall be allowed to register them, as per CRA-N001.  BM Units are related to GSP Groups, Interconnectors and Boundary Points dependent upon the type of the BM Unit. The CRA system shall maintain the relationship between a BM Unit and either a GSP Group or Interconnector, but not a Boundary Point. The following table illustrates which BM Unit types require an association to a GSP Group / Interconnector to be specified.    A BM Unit registration request shall contain the following information:   An Action Description   The BM Unit Registration Details (including type, production / consumption flag and whether an SO defined name is contained within the flow)   Generation Capacity and Demand Capacity   Details of the GSP group associated with the BM Unit (if appropriate)   Details of the Interconnector associated with the BM Unit (if appropriate)   Whether the BM Unit is part of a group of related BM Units (Joint BM Unit details) and where appropriate, the other BM Units in the group.   Mapping Details defining the relationships between SVA MSIDs and the BM Unit   FPN Flag for the BM Unit   Base TU Flag   Joint BM Unit Flag  A detailed description of the interface content may be found in CRA-I005.  The CRA shall accept updated details of the registration from BSCCo Ltd including:   Exempt Export Flag   Manual Credit Qualifying Flag  A detailed description of the interface content may be found in CRA-I043.  The system shall validate the following details:  1) That the referenced lead Party is contained within the system and is a currently valid BSC Party and not a Party Agent  2) That the GSP Group referenced is contained within the system (where appropriate for type)  3) That the Interconnector referenced is contained within the system (where appropriate for type)  4) That the name provided for the BM unit is not duplicated within the system  5) That the sending BSC Party is of a type able to register a BM Unit as specified in the mapping between BSC Party types and Registration operations  6) That a valid (not null) WDCALF and NWDCALF value has been received (see CRA-F020) and entered  7) That if the BM Unit is a “Supplier BM Unit”, then a valid (not null) SECALF value has been received (see CRA-F020) and entered  8) That if the BM Unit is a “Supplier BM Unit”, then the Effective To Date for the BM Unit is open ended.  Where a duplicate name is found, the system shall warn the Operator of the fact and ask for confirmation before further processing. Where the last check is failed, the Operator shall be presented with a warning which must be explicitly overridden prior to acceptance of the data.  **Production / Consumption Flag**  Should the Production / Consumption flag be set within the flow, it is the responsibility of the Operator to ensure that an authorisation to support this has been received from BSCCo Ltd. The CRA system shall not allow the Production / Consumption Flag to be set for a non-Exempt Export BM Unit (unless it is an Interconnector User BM Unit, in which case the flag must be set).  In the case of an Exempt Export BM Unit, the Production / Consumption flag shall always be set to either “Production” or “Consumption” and shall never be cleared by the Operator while the BM Unit has Exempt Export status.  **Exempt Export Flag[[4]](#footnote-5)**  On registration, the Exempt Export Flag shall be unset by default for all BM Units.  **Manual Credit Qualifying Flag**  BSCCo may instruct the Service Provider to change the value of the Manual Credit Qualifying Flag at the time of registration. A default value of 'False' will be used where no value is specified.  **Base TU Flag**  On registration, the Base TU Flag shall be set by default for all Base Supplier BM Units and Additional Supplier BM Units to indicate that the BM Unit is allocated to the GSP Group Base Trading Unit. The Base TU Flag shall be unset by default for all non-Exempt Export Embedded BM Units. The CRA system shall not allow the Base TU flag to be set for Directly Connected or Interconnector User BM Units.  After all validation has been completed, the system shall return a new unique, meaningful identifier for the BM Unit on completion of storing the registration data. Where an NGC BM Unit name is supplied, this shall be stored against the BM Unit, though the name shall not be considered when generating the NETA BM Unit Identifier. In addition, the event shall trigger the creation of a Trading Unit for the BM Unit in accordance with the requirement of CRA-F015.  Where registration is accepted, the system shall calculate the WDBMCAEC, NWDBMCAEC, WDBMCAIC, NWDBMCAIC and Production / Consumption statusand trigger the sending of a BM Unit, Interconnector and GSP Group Data (CRA-I015) report and a Registration Report (CRA-I014).  The CRA may from time to time issue the Credit Assessment Capability (CRA-I017) report to the SAA and ECVAA.  The calculation of the Production / Consumption status will only be conducted where the Production / Consumption flag is not set on reception from the BSC Party. Where the Base TU Flag is set and the Production / Consumption flag is null, the Production / Consumption status of a BM Unit shall be set to “Consumption” by default. Note that the Production / Consumption flag cannot be set to null for an Exempt Export BM Unit.  Where the requirement functionality has been triggered from CRA-F001 or CRA-F030 in order to create a “Supplier BM Unit”, a subset of the CRA-I015 output data flow shall be sent to the SVAA.  Where the input details state a relationship between a BM Unit and one or many SVA MSIDs, the system shall store the relationship and issue a report on the mapping to the SMRA through CRA-I023.  The creation of a Joint BM Unit Group shall require the approval of BSCCo Ltd. The creation of Joint BM Unit Groups will involve both the BSC Party and the SO. The BSC Party will submit appropriate evidence to confirm SO authorisation when requesting the registration, this may be in the form of a letter, fax or any other suitable means.  Where the interface specifies the creation of a Joint BM Unit Group, the system shall validate that each of the BM Units in the Group have been previously registered in the CRA system.  Where the registration is indicated as part of a transfer to or from SMRA, then   If confirmation of the transfer has been received from the transfer coordinator:  - Enter the data ensuring the confirmed date is used as this may differ from that originally submitted.  - Send an extract of the entered data to the transfer coordinator.   Where confirmation has not been received:  - Carry out validation but do not enter the data.  - Send a copy of the request to the transfer coordinator. | | | |
| A BM Unit will be considered as having a Credit Qualifying Status of “True” for those effective Settlement Dates where it meets the following conditions:   It is not an Interconnector BM Unit; and   Its FPN Flag set as “True”; and   Either:  1. It is an Exempt Export BM Unit; or  2. It has a Production/Consumption Flag set as “Production”; or  3. It has a Manual Credit Qualifying Flag set as “True”.  For all other effective Settlement Dates a BM Unit will be considered as having a Credit Qualifying Status of “False”. | | | |
| A BM Unit will have its Demand-in-Production Flag set as “True” for those effective Settlement Dates where it meets the following conditions:   It is not an Exempt Export BM Unit; and   It has a Credit Qualifying Status of “False”; and   It has a Production/Consumption Flag set as “Production”; and   Its Relevant Capacity is not greater than zero (i.e. GCi + DCi <= 0).  For all other effective Settlement Dates a BM Unit’s Demand-in-Production Flag set as “False”. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I005  Output interfaces:  CRA-I014  CRA-I015  CRA-I017  CRA-I019  CRA-I020  CRA-I023  CRA-I028 | | | |

## 5.14 CRA-F014: View / Maintain BM Unit Registration

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F014 | **Status:**  Mandatory | **Title:**  View / Maintain BM Unit Registration | **BSC Reference:**  CRA SD 6.1, CRA BPM 3.2, NGC VAL 3.0, CRAWS-34, CRAWS‑37, DID‑2, CP775, P100, P215, P268, P269 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low (A few per month) | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to view and amend the details of a BM Unit registration within the system.  The CRA shall accept updated details of the registration from the BSC Party or BSCCo (as set out in CRA-F041 & CRA-F043) including:   The BM Unit Registration Details (including type, production / consumption flag and whether an SO defined name is contained within the flow)   s QMij(for conversion to Generation Capacity) and Negative QMij (for conversion to Demand Capacity)   Details of the GSP group associated with the BM Unit (if appropriate)   Details of the Interconnector associated with the BM Unit (if appropriate)   Whether the BM Unit is part of a group of related BM Units and, where appropriate, the other BM Units in the group.   MPAN - BM Unit mapping Details   BM Unit FPN Flag   Base TU Flag   Joint BM Unit Flag  A detailed description of the interface content may be found in CRA-I005.  The CRA shall accept updated details of the registration from BSCCo Ltd including:   Exempt Export Flag   Manual Credit Qualifying Flag  A detailed description of the interface content may be found in CRA-I043.  The Operator shall be able to:  1) Amend the details of the BM Unit - type (production / consumption), generation capacity, location and name,  2) Change the lead Party for the BM unit,  3) Amend the list of MPANs associated with the BM Unit.  4) Amend the Joint BM Unit details.  The following sections detail the constraints under which each of the operations may be conducted. | | | |
| Where a BM Unit’s name is changed, the CRA system shall issue a warning to the Operator and ask for explicit confirmation of the change of name.  Where the NGC BM Unit Name is changed, the system shall update the BM Unit with the new name, and the date of the change.  Where Generation Capacity is decreased or Demand Capacity is increased within a BSC Season, the CRA system shall issue a warning to the Operator and ask for explicit confirmation of the change. This would be allowed only if authorisation for the change has been received from BSCCo Ltd.  The WDCALF, NWDCALF and SECALF values (see CRA-F020) cannot be set to NULL for a current BM Unit.  If the BM Unit is a “Supplier BM Unit” that was originally created as a result of a trigger from CRA-F001 or CRA-F030 (i.e. it is a “Base BM Unit”), the CRA system will ensure that the Effective Date Range of the BM Unit is contiguous and open ended. If it is not, then the CRA system shall issue a warning to the Operator to ask for explicit confirmation of the change. This should generally be allowed only if:  1. the BM Unit is being de-registered as a result de-registration of the associated BSC Party or GSP Group, i.e. the Effective To Date is changed from open ended to a specified date,  2. the BM Unit is being re-registered following de-registration, i.e. the Effective From Date of the new record is after the Effective To Date of an existing record.  Where the Lead Party is being changed, that the referenced lead Party is contained within the system and is a currently valid BSC Party and not a Party Agent  Where the generation capacity or demand capacity of the BM Unit is changed the system shall calculate the WDBMCAEC, NWDBMCAEC, WDBMCAIC and NWDBMCAIC, and trigger the sending of a BM Unit, Interconnector and GSP Group Data (CRA-I015) report and a Registration Report (CRA-I014)  The CRA may from time to time issue the Credit Assessment Capability (CRA-I017) report to the SAA and ECVAA.  Generation Capacity and Demand Capacity data, and Production / Consumption information may be resubmitted to the CRA at any time by the relevant Parties. However, it will be necessary for the Parties to submit the information at least one working day in advance of when the change will take effect.  Should the Production / Consumption flag be set within the flow, it is the responsibility of the Operator to ensure that an authorisation to support this has been received from BSCCo Ltd. The CRA system shall allow the Production / Consumption Flag to be changed for any Exempt Export BM Unit. The CRA system shall not allow the Production / Consumption Flag to be set for a non-Exempt Export BM Unit (unless it is an Interconnector User BM Unit, in which case the flag must be set).  In the case of an Exempt Export BM Unit, the Production / Consumption flag shall always be set to either “Production” or “Consumption” and shall never be cleared by the Operator while the BM Units retains its Exempt Export status.  Subsequently, this information shall be issued through interface CRA-I017. | | | |
| The CRA system shall allow an Operator to view and update the Exempt Export Flag for a BM Unit.  The CRA system shall only allow the Exempt Export Flag to be changed for Base Supplier BM Units, Additional Supplier BM Units, Embedded BM Units and Directly Connected BM Units. The CRA system shall not allow the Exempt Export Flag to be changed for any other type of BM Unit.  Where a request to change the Exempt Export Flag of a Base Supplier BM Unit or Additional Supplier BM Unit indicates that the BM Unit is to be non-Exempt Export (and therefore, re-allocated to the GSP Group Base Trading Unit), the CRA shall validate that the BM Unit does not belong to an explicit Trading Unit already. If it does, the request shall be rejected.  Where a valid request to change the Exempt Export Flag indicates that the BM Unit is to be Exempt Export, the CRA shall set the Exempt Export Flag.  Where a valid request to change the Exempt Export Flag indicates that the BM Unit is to be non-Exempt Export, the CRA shall:  1. clear the Production / Consumption Flag to indicate that Production / Consumption Status is derived dynamically  2. for Base Supplier BM Units and Additional Supplier BM Units, set the Base TU Flag to indicate that the BM Unit is allocated to the GSP Group Base Trading Unit  3. for all other BM Units, unset the Base TU Flag and allocate the BM Unit to its own (default) Trading Unit  4. unset the Exempt Export Flag.  The new Exempt Export Flag shall subsequently be distributed as per the requirements of CRA-I014 and CRA-I020. | | | |
| The CRA system shall allow for the transfer of responsibility of a BM Unit from one lead Party to another. However, if the BM Unit is of a Supplier BM Unit, a warning shall be issued to the Operator.  The process of responsibility transference shall be a multi-step process conducted in the following manner:  Where a Party informs the CRA of responsibility for a BM Unit currently allocated to another Party, the CRA shall inform the Operator of this fact. The Operator must acknowledge this warning, upon which, the details of the registration change shall be stored within the system in a pending state. Should the effective start date by sooner than a predefined, system defined time limit [28 days]. The Operator shall also be warned of the fact.  On completion of the update an acknowledgement of the registration request will be sent to both the new and old Parties.  Where subsequently, a confirmation of the transference is sent from the old Party, the CRA system shall validate that the effective to date from the new Party is consistent with that received from the new Party. Where this occurs, the system shall update both the pending registration and the new registration.  Where the confirmation of responsibility is received after the effective start date of the new registration, the system shall present the Operator with a warning. This must be explicitly overridden by a Supervisor prior to the update being conducted. Where the Supervisor decides that the update cannot take place, the new registration request may also be put in a pending state for later resolution.  The change of BM Unit responsibility shall not require a change in BM Unit name. | | | |
| Where the input details state a change to the relationship between a BM Unit and one or many Stage 2 MPAN’s, the system shall store the amended relationship and issue a report on the mapping to the SMRA through CRA-I023. | | | |
| Where a request to change the Base TU Flag is received the CRA shall validate that the BM Unit is Exempt Export and, if not, the request shall be rejected.  The CRA system shall not allow the Base TU Flag to be changed for Directly Connected or Interconnector User BM Units.  Where a request to change the Base TU Flag indicates that the BM Unit is to be allocated to the GSP Group Base Trading Unit, the CRA shall validate that the BM Unit does not belong to an explicit Trading Unit already. If it does, the request shall be rejected.  Where a valid request to change the Base TU Flag indicates that the BM Unit is to be added to the GSP Group Base Trading Unit, the CRA shall re-allocate the BM Unit from its own (default) Trading Unit to the GSP Group Base Trading Unit.  Where a valid request to change the Base TU Flag indicates that the BM Unit is to be removed from the GSP Group Base Trading Unit, the CRA shall re-allocate the BM Unit to its own (default) Trading Unit.  Allocations and de-allocations to/from a GSP Group Base Trading Unit shall be made via the Base TU Flag only.  The Production / Consumption Status of the Base Trading Unit and its components shall be re‑computed for each change to a Base TU Flag. Where the Base TU Flag is set and the Production / Consumption flag is null, the Production / Consumption status of a BM Unit shall be set to “Consumption” by default. Note that the Production / Consumption flag cannot be set to null for an Exempt Export BM Unit. | | | |
| The CRA system shall allow for the amendment of a Joint BM Unit through either the addition or subtraction of BM Units. | | | |
| A BM Unit will be considered as having a Credit Qualifying Status of “True” for those effective Settlement Dates where it meets the following conditions:   It is not an Interconnector BM Unit; and   Its FPN Flag set as “True”; and   Either:  1. It is an Exempt Export BM Unit; or  2. It has a Production/Consumption Flag set as “Production”; or  3. It has a Manual Credit Qualifying Flag set as “True”.  For all other effective Settlement Dates a BM Unit will be considered as having a Credit Qualifying Status of “False”. | | | |
| A BM Unit will have its Demand-in-Production Flag set as “True” for those effective Settlement Dates where it meets the following conditions:   It is not an Exempt Export BM Unit; and   It has a Credit Qualifying Status of “False”; and   It has a Production/Consumption Flag set as “Production”; and   Its Relevant Capacity is not greater than zero (i.e. GCi + DCi <= 0).  For all other effective Settlement Dates a BM Unit’s Demand-in-Production Flag set as “False”. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I005  CRA-I009  CRA-I043  Output interfaces:  CRA-I014  CRA-I015  CRA-I017  CRA-I019  CRA-I020  CRA-I023  CRA-I028 | | | |

## 5.15 CRA-F015: Trading Unit Registration

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F015 | **Status:**  Mandatory | **Title:**  Trading Unit Registration | **BSC Reference:**  CRA SD 6.2, CRA BPM 3.2, CRAWS-35, P100 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to enter details of a Trading Unit registration into the system (excluding Base Trading Units). The information for the definition of the Trading Unit shall be composed of:   An Action Description   Trading Unit Details (name, registration dates)   Component BM Units  The definition of a Trading Unit requires the explicit authorisation of BSCCo Ltd. It shall be the responsibility of the Operator to ensure that supporting documentation from BSCCo Ltd has been received and are consistent with the Trading Unit registration request.  Trading Units should only be created by BSC Traders though other Parties shall not be restricted in their creation as per CRA-N001.  The system shall validate the following details:  1) That each of the BM Units acceptance of commercial responsibility is registered and recorded within the CRA system.  2) That at least one BM Unit is listed as a component of the Trading Unit (by default, on creation of a BM Unit, a Trading Unit is defined for the BM Unit).  3) That Base Supplier BM Units and Additional Supplier BM Units are Exempt Export.  After all validation has been completed, the system shall return a new unique identifier for the Trading Unit on completion of storing the registration data.  Where a BM Unit is associated with a Trading Unit explicitly, any previous association with a Trading Unit will be removed. This includes removal from a GSP Group Base Trading Unit, which the CRA shall perform according to requirement CRA-F014. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I006  Output Interfaces:  CRA-014  CRA-I015  CRA-I019  CRA-I020 | | | |

## 5.16 CRA-F016: View / Maintain Trading Unit Registration Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F016 | **Status:**  Mandatory | **Title:**  View / Maintain Trading Unit Registration Details | **BSC Reference:**  CRA SD 6.2, CRA BPM 3.2, CRAWS-35, CRAWS-39 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to enter details of Trading Unit registration changes into the system. The information for the amendment of the Trading Unit shall be composed of:   An Action Description   Trading Unit Details (name, registration dates)   Component BM Units  Any change to a Trading Unit registration requires the explicit authorisation of BSCCo Ltd  The system shall validate that each of the BM Units’ acceptance of commercial responsibility is registered and recorded within the CRA system.  Where a BM Unit is removed from a Trading Unit, it shall be reassigned to its own (default) Trading Unit after completion of the operation. Where a BM Unit is added to a Trading Unit, it shall be removed from its (default) Trading Unit.  Where a change to the scope of the component BM Units (either through addition or subtraction) fails validation, the Trading Unit registration request will be held as pending subject to resolution. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I006  Output Interfaces:  CRA-I014  CRA-I015  CRA-I019  CRA-I020 | | | |

## 5.17 CRA-F017: Register CRA Boundary Points and System Connection Points Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F017 | **Status:**  Mandatory | **Title:**  Register CRA Boundary Points and System Connection Points Details | **BSC Reference:**  CRA SD 6.4, CRA BPM 3.3, CR\_990813\_07, CRAWS-36, CRAWS-39, CP615, CP1301 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| 1. The CRA shall register data relating to all Boundary Points and System Connection Points. These are registered by either the System Operator or a Distribution System Operator using flow CRA-I007 at least 20 WD before the Effective From date. The BSCP form on which this flow is based contains additional information which is not captured in the database, but which is used by other recipients of the form.  a. A Boundary Point is a point at which any Plant or Apparatus not forming part of the Total System is connected to the Total System (Total System means the Transmission System and each Distribution System)  Boundary Points Registered By System Operator are:   Gensets directly connected to the Transmission Network   Station Transformers directly connected to the Transmission Network   Demand sites directly connected to the Transmission Network   Interconnectors with other Transmission Systems  Boundary Points Registered by the Distribution Business are:   Embedded sites, under the direct control of the System Operator, that form an individual BM Unit. (These are sites over 50 MW or those being despatched by the System Operator).   Other Embedded sites.   Interconnectors with other Transmission Systems (where these connect to a distribution system)  b. A System Connection Point is a point at which two or more Systems are connected, including a connection between Distribution Systems in different GSP Groups (but excluding a connection between Distribution Systems in the same GSP Group).  System Connection Points Registered By System Operator are:   Grid Supply Points (including Offshore Transmission Connection Points)   An Offshore Transmission Connection Point is a point where a Distribution System connects to an Offshore Transmission System and will be registered by the System Operator as a Grid Supply Point.  System Connection Points Registered By Distribution Business are:   Interconnectors Between Distribution Networks  2. In each case CRA shall maintain the following information:   Boundary Point, or System Connection Point Identifier;   Boundary Point or System Connection Point Type   Effective From Date   Effective To Date  3. Where a request is received to create a Boundary Point or System Connection Point then CRA shall inform BSCCo Ltd by forwarding a copy of the information provided. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I007  Output Interfaces:  CRA-I007  CRA-I014  CRA-I019  CRA-I028 | | | |
| **Issues:** | | | |
|  | | | |

## 5.18 CRA-F034: Register Metering System Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F034 | **Status:**  Mandatory | **Title:**  Register Metering System Details | **BSC Reference:**  CRA SD 6.4, CRA BPM 3.3, CR\_990813\_07, CRAWS-36, CRAWS-39, CP569, CP753, P55, CP1301 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall receive the following information concerning the registration of Boundary Points and Metering Systems.   An Action Description   Authentication Details   Metering System Details (including the Meter Operator Agent for the Metering System)  Metering Systems should only be registered by certain types of BSC Parties. The following table illustrates which type of BSC Party should register a Metering System(See CRA-N001)  cp1301 pic  The System Operator shall register Metering System details for Offshore Transmission Connection Points only. All other Metering Systems for Grid Supply Points shall be registered by the Distribution Company.  It shall be the responsibility of the Operator to ensure that the type of the meter specified on the incoming flow is correct against any supporting paper based documentation.  Where metering system details are registered, the CRA shall validate that the Meter Operator Agent specified against the metering system is registered with the CRA.  Where a Metering System is attempted to be registered but already exists within the system, the Operator shall be informed of the event and may, instead, enter the new details as an amendment to the current details through the View / Maintain Metering Systems functionality.  For each new Metering System registration, the CRA shall ensure that the registrant has confirmed that either:   the Registrant is the Equipment Owner, or   the Registrant has obtained the Equipment Owner’s consent for the appointment.  Where the registration is indicated as part of a transfer to or from SMRA, then   If confirmation of the transfer has been received from the transfer coordinator:  - Enter the data ensuring the confirmed date is used as this may differ from that originally submitted.  - Send an extract of the entered data to the transfer coordinator.   Where confirmation has not been received:  - Carry out validation but do not enter the data. If necessary allocate a Metering System Identifier and inform the registrant.  - Send a copy of the request, including any allocated metering system id, to the transfer coordinator. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I031  Output Interfaces:  CRA-I014  CRA-I019  CRA-I022  CRA-I028 | | | |
| **Issues:** | | | |
|  | | | |

## 5.19 CRA-F018: View / Maintain Boundary Point and System Connection Point Details

| **Requirement ID:**  CRA-F018 | **Status:**  Mandatory | **Title:**  View / Maintain Boundary Points Details | **BSC Reference:**  CRA SD 6.4, CRA BPM 3.3, CRAWS-36, CRAWS-37, CRAWS-39 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall receive changes to the registration of Boundary Points and System Connection Points.  Where a request is received to decommission a Boundary Point or System Connection Point then CRA shall inform BSCCo Ltd by forwarding a copy of the information provided. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I007  Output Interfaces:  CRA-I014  CRA-I019  CRA-I028 | | | |

## 5.20 CRA-F019: View / Maintain Interconnector Registration

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F019 | **Status:**  Mandatory | **Title:**  View / Maintain Interconnector Registration | **BSC Reference:**  CRA SD 6.3, CRA BPM 3.6, CRAWS-38, CRAWS-39 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to register Interconnector Registration details. The details of an Interconnector shall be composed of:   Action Description   Authentication Details   Interconnector Details (including GSP group where appropriate) | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I008  Output Interfaces:  CRA-I014  CRA-I015  CRA-I020 | | | |

## 5.21 CRA-F020: Maintain Credit Assessment Load Factor

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F020 | **Status:**  Mandatory | **Title:**  Maintain Credit Assessment Load Factor | **BSC Reference:**  CRA SD 7.1, CRA SD 7.2, CRA BPM 2, CR012, CP775, P310 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to view and update the Working Day Credit Assessment Load Factor (WDCALFi), Non-Working Day Credit Assessment Load Factor (NWDCALFi) and Supplier Export Credit Assessment Load Factor (SECALFi) values for a BM Unit. The Working Day Credit Assessment Load Factor (WDCALFi), Non-Working Day Credit Assessment Load Factor (NWDCALFi) and SECALFi are each single values per BM Unit that may be changed from time to time. SECALFi values are only relevant for Supplier BM Units; for all other BM Units a zero value of SECALFi shall be entered.  The interface contains the following information:   Action Description   Authentication Details   WDCALFi and date from which it is effective.  • NWDCALFi and date from which it is effective.   SECALFi and date from which it is effective.  The WDCALFi, NWDCALFi and SECALFi values cannot be set to NULL for a current BM Unit.  At the effective commencement date of the new BM Unit WDCALFi, NWDCALFi or SECALFi, the CRA shall recalculate the Working Day BM Unit Credit Assessment Export Capability (WDBMCAECi) , the Non-Working Day BM Unit Credit Assessment Export Capability (NWDBMCAECi), the Working Day BM Unit Credit Assessment Import Capability (WDBMCAICi) and the Non-Working Day BM Unit Credit Assessment Import Capability (NWDBMCAICi) in accordance with the following formula for all registered BM Units:  WDBMCAICi = WDCALFi\*DCi  NWDBMCAICi = NWDCALFi\*DCi  If Supplier BM Unit,  If DCi=0 and GCi>0, then  WDBMCAECi = SECALFi\*GCi  NWDBMCAECi = SECALFi\*GCi  Else  WDBMCAECi = WDCALFi\*GCi  NWDBMCAECi = NWDCALFi\*GCi  The new WDBMCAECi, NWDBMCAECi, WDBMCAICi and NWDBMCAICi for all BM Units shall subsequently be distributed as per the requirements of CRA-F013 and CRA-F014.  The CRA may from time to time issue the Credit Assessment Capability Report (CRA-I017) to the SAA and ECVAA Services. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I011  Output Interfaces:  CRA-I014  CRA-I015  CRA-I017 | | | |

## 5.22 CRA-F021: Requirement not currently used

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F021 | **Status:** | **Title:**  Requirement not currently used | **BSC Reference:** |
| **Man/Auto:** | **Frequency:** | **Volumes:** | |
| **Functional Requirement:** | | | |
|  | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.23 CRA-F022: Issue Credit Assessment Capability

| **Requirement ID:**  CRA-F022 | **Status:**  Mandatory | **Title:**  Issue Credit Assessment Capability | **BSC Reference:**  CRA SD 7.1, CRA SD 7.2, CRA BPM 2, CR012, P100, P310 |
| --- | --- | --- | --- |
| **Man/Auto:**  Automatic | **Frequency:**  Monthly or Ad-hoc | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall recalculate and store the Working Day BM Unit Credit Assessment Export Capability (WDBMCAECi), the Non-Working Day BM Unit Credit Assessment Export Capability (NWDBMCAECi), the Working Day BM Unit Credit Assessment Import Capability (WDBMCAICi) and the Non-Working Day BM Unit Credit Assessment Import Capability (NWDBMCAICi) in accordance with the following formula for all registered BM Units once per month or for individual BM Units when triggered as a result of the:   redefinition of a Trading Unit;   registration of a new BM Unit;   change in the Generation or Demand Capacity for a BM Unit   change in the WDCALFi, NWDCALFi or SECALFi for a BM Unit  The CRA shall calculate the Credit Assessment Capability values as:  WDBMCAICi = WDCALFi\*DCi  NWDBMCAICi = NWDCALFi\*DCi  If Supplier BM Unit,  If DCi=0 and GCi>0, then  WDBMCAECi = WDSECALFi\*GCi  NWDBMCAECi = SECALFi\*GCi  Else  WDBMCAECi = CALFi\*GCi  NWDBMCAECi = NWDCALFi\*GCi  The system shall not overwrite the previous values of the WDBMCAECi, NWDBMCAECi, WDBMCAICi or NWDBMCAICi, but log the new data with the date from which it is effective.  The CRA shall also recalculate the Production / Consumption Status for the affected BM Units if the BM Unit is defined to have a non-fixed Production / Consumption Status, as follows:  If DCi >= GCi, then  the Relevant Capacity is DCi.  Else  the Relevant Capacity is GCi.  The Trading Unit Production / Consumption Status is determined by summing the Relevant Capacities for all BM Units in the Trading Unit.  If the sum of the Relevant Capacities is <= 0, then  the Trading Unit Status is Consumption  else  the Trading Unit Status is Production.  Each BM Unit shall be assigned the same (Production / Consumption) Status as the relevant Trading Unit, except in the case where the Flag has been notified by the Party. In this case, the BM Unit Production/Consumption Status is as notified by the Party (Production / Consumption Flag set).  The CRA will distribute the new WDBMCAECi, NWDBMCAECi, WDBMCAICi and NWDBMCAICi for all BM Units as per the requirements of CRA-F013 and CRA-F014. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Output Interfaces:  CRA-I014  CRA-I015  CRA-I017 | | | |

## 5.24 CRA-F023: Validate Registrations

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F023 | **Status:**  Mandatory | **Title:**  Validate Registrations | **BSC Reference:**  CRA SD 8, CRA BPM 3.4, CRAWS-40, P100 |
| **Man/Auto:**  Automatic | **Frequency:**  Daily | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall on a daily basis, perform a validation check to ensure the consistency of all data that has been changed over the course of the day. This check shall highlight conditions in two states - Error and Warning and shall validate that:  1) All BM Units are associated with a Trading Unit, (Error)  2) All Interconnectors have a defined Interconnector Error Administrator. In addition that the BSC Party statement of Error Administrator registration matches that received through the Interconnector Administrator registration data. (Warning / Error)  3) That all BM Units have a defined lead Party (Error)  4) That no BM unit responsibility registration requests are pending (Warning)  5) That all BSC Party and Service Agents are outside of a system wide time prior to the end of their certification period [28 days] (Warning)  6) That there are no unconfirmed change of BM Unit responsibility requests within a system wide period of the date of change. [28 days] (Warning)  7) All Base Supplier BM Units and Additional Supplier BM Units that are not Exempt Export, are allocated to the Base Trading Unit of the appropriate GSP Group (Warning).  In addition, the CRA system shall list all registration changes that are pending or failed along with the date at which they entered such states.  The system shall present each validation warning / failure to the Operator through an online screen on demand for subsequent rectification through View / Maintain functionality described in previous appropriate requirements.  The CRA system shall allow an Operator to search through the highlighted information by failure type, BSC Party and effective to / from dates to limit the amount of information presented at any one time. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.25 CRA-F024: Report Registration Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F024 | **Status:**  Mandatory | **Title:**  Report Registration Details | **BSC Reference:**  CRA SD 10, CRA BPM 3.7, CRAWS-41 |
| **Man/Auto:**  Automatic | **Frequency:**  Daily | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall produce a report, daily, on all registration details that have changed over the course of the day to the relevant BSC Parties.  The system shall maintain a log of all information distributed on each occurrence. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Output Interfaces:  CRA-I014 | | | |

## 5.26 CRA-F025: Distribute Register Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F025 | **Status:**  Mandatory | **Title:**  Distribute Register Data | **BSC Reference:**  CRA SD 10, CRA SD 11, CRA BPM 3.8, CRAWS-42, CR\_991027\_06a, CP753, CP551, CP642, P197 |
| **Man/Auto:**  Automatic | **Frequency:**  See Text | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall, daily (or more frequently if multiple changes occur), distribute changes to centrally held register data within the system on a pre-defined schedule. The following data shall be distributed daily as a result of a change to the base data as highlighted in prior requirements:  CRA-I013 - Issue Authentication Report  CRA-I014 - Issue Registration Report  CRA-I015 - Issue BM Unit & Energy Account Registration Data (See Note 1)  CRA-I017 - Issue Credit Assessment Capability  CRA-I020 - Issue Operations Registration Report (Incremental Report)  CRA-I022 - Issue Metering System Details  CRA-I024 - Issue Certification & Accreditation Status Report[[5]](#footnote-6)  CRA-I028 - Issue NGC Standing Data Report  The following data shall be distributed monthly irrespective of whether the data has changed over the previous month.  CRA-I013 - Issue Authentication Report  CRA-I017 - Issue Credit Assessment Capability  The following data shall be sent to the BSCCo weekly irrespective of whether the data has changed over the previous week:  CRA-I020 - Issue Operations Registration Report (Full Refresh Report)  Each report shall also be able to be distributed on request through an Operator entering the distribution details.  Note 1: The BM Unit and Energy Account Registration report (CRA-I015, subflow 2) generated for SVAA will only be sent if the report itself differs from the previously generated report. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Output Interfaces:  CRA-I013  CRA-I014  CRA-I015  CRA-I017  CRA-I020  CRA-I022  CRA-I024  CRA-I028 | | | |

## 5.27 CRA-F026: Maintain Reference Data

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F026 | **Status:**  Mandatory | **Title:**  Maintain Reference Data | **BSC Reference:**  CRA SD 8, CR\_990813\_07, CRAWS-43 |
| **Man/Auto:**  Manual | **Frequency:**  Daily | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA system shall provide facilities for the maintenance of reference data used within the system. The following data shall be maintained (though additional requirements may be found during detailed design):  a) BSC Party Types,  b) BSC Party Agent Types,  c) BSC Service Agent Types,  d) Settlement Report Distribution Methods,  e) Point Types,  f) BM Unit Types. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| The information is expected to be presented to the CRA system in low volume on paper. | | | |

## 5.28 CRA-F027: SLA Reporting

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F027 | **Status:**  Mandatory | **Title:**  SLA Reporting | **BSC Reference:**  CRA SD Appendix B, CRAWS-45, P197, P310 |
| **Man/Auto:**  Manual | **Frequency:**  Monthly | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall produce reports monthly detailing the level of service provided by the Service to the BSCCo Ltd. The reports shall detail the response times in delivering various aspects of the system as detailed below. The Service level for each of the activities is contained within the brackets in each case.  Other General requirements are described within the Common requirement GEN-N005  1) Process New BSC Party registrations - Validate data, authenticate registration application and update registration system with new registration data on the Working Day received (100%).  2) Process Change to BSC Party Standing Data - Validate changes to data and update registration system with new data on the Working Day received (100%)  3) Provide BSC Party Registration report - Registration reports produced and despatched to recipient on the Working Day received (100%)  4) BSC Party Authentication Details - Reports produced and despatched to recipient on the Working Day received(100%)  5) Qualify new BSC Party Agent - Complete Qualification Report returned on the Working Day received(100%)  6) Credit Assessment Import/Export Capability re-set on a monthly basis or within [1 Working Day] of change to WDCALF, NWDCALF or SECALF or DC or GC (100%) | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| BSCCo Ltd | | | |

## 5.29 CRA-F028: Requirement not currently used

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F028 | **Status:** | **Title:**  Requirement not currently used | **BSC Reference:** |
| **Man/Auto:** | **Frequency:** | **Volumes:** | |
| **Functional Requirement:** | | | |
|  | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.30 CRA-F029: Register Interconnector

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F029 | **Status:**  Mandatory | **Title:**  Register Interconnector | **BSC Reference:**  CRA SD 6.3, CRA BPM 3.6, CRAWS-38 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to register Interconnector Registration details. The details of an Interconnector shall be composed of:   Action Description   Authentication Details   Interconnector Details (including GSP group where appropriate)  Interconnectors should only be registered by a limited sub-set of BSC Parties (the Transmission Owner / Distribution Company) though other BSC Party types may register them in accordance with CRA-N001.  Interconnectors may only be registered after endorsement from BSCCo Ltd. It shall thus be the responsibility of the Operator to ensure that supporting documentation has been received and checked prior to registration. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I008  Output Interfaces triggered from this activity:  CRA-I014  CRA-I015  CRA-I020 | | | |

## 5.31 CRA-F030: Register GSP Group and GSP Details

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F030 | **Status:**  Mandatory | **Title:**  Register GSP Group and GSP Details | **BSC Reference:**  CRAWS-44, P100 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to register GSP Group, GSP and Distribution Systems Connection Point (DSCP) Registration details. The details of a GSP Group shall be composed of:   Action Description,   Authentication Details,   GSP Group Details,   GSP Details,  GSP Groups should only be registered by a limited sub-set of BSC Parties (The Distribution Companies) though other Party types may register in accordance with CRA-N001.  GSP Groups may only be registered after endorsement from BSCCo Ltd. It shall thus be the responsibility of the Operator to ensure that supporting documentation has been received and checked prior to registration. The CRA system shall allow the Operator to enter details that these checks have been conducted.  On successful registration of a GSP Group, the CRA shall register a Base Trading Unit for that GSP Group (with CRA as the registrant). Each BSC Party of type “Supplier” shall be returned a BM Unit of type “Base Supplier BM Unit” in accordance with the requirements of CRA-F013. Each Base Supplier BM Unit created in this way shall, by default, be allocated to the GSP Group Base Trading Unit, in accordance with the requirements of CRA-F013.  The CRA shall not maintain an association between GSP Groups and GSPs. This shall be the responsibility of the CDCA, where required. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I027  Output Interfaces:  CRA-I014  CRA-I028 | | | |

## 5.32 CRA-F031: View / Maintain GSP Group Registrations

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F031 | **Status:**  Mandatory | **Title:**  View Maintain GSP Group and GSP Registrations | **BSC Reference:**  CRAWS-44 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to register changes to the GSP Group Registration details. The details of a GSP Group shall be composed of:   Action Description,   Authentication Details,   GSP Group Details,   GSP Details,   GSP Registrant.  Changes to GSP Groups may only be registered after endorsement from BSCCo Ltd. It shall thus be the responsibility of the Operator to ensure that supporting documentation has been received and checked prior to registration. The CRA system shall allow the Operator to enter details that these checks have been conducted. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I027  Output Interfaces:  CRA-I014  CRA-I019  CRA-I028 | | | |

## 5.33 CRA-F032: Maintain Transmission Loss Factors

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F032 | **Status:**  Mandatory | **Title:**  Maintain Transmission Loss Factors | **BSC Reference:** |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall allow an Operator to update the Transmission Loss Factors for a BM Unit when instructed from BSCCo Ltd.  BSCCo Ltd shall provide the following information:   The Proportion of Losses (alpha)   The Transmission Loss Factors for individual BM Units for each Settlement Day.  The CRA system shall validate that each BM Unit detailed is registered for the range of effect of the Transmission Loss Factor Update. Where a discrepancy is found, the system shall issue a warning to the Operator.  The Transmission Loss Factors shall be issued via the CRA-I015. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I029  Output Interfaces:  CRA-I015 | | | |

## 5.34 CRA-F033: Receive Registration Exception Reports

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F033 | **Status:**  Mandatory | **Title:**  Receive Registration Exception Reports | **BSC Reference:** |
| **Man/Auto:**  Automatic | **Frequency:**  As Necessary | **Volumes:**  Infrequent | |
| **Functional Requirement:** | | | |
| The CRA system shall receive Exception reports from the SAA, BMRA and ECVAA systems where Registration data sent to these systems has been rejected.  The CRA system shall receive exception data including:   Sending Agent   Exception Type   Exception Description  The CRA system shall receive the exceptions automatically and allow an Operator to view the nature and description of the Exception. It is subsequently the responsibility of the Operator or a Supervisor to communicate with the sending Agent and resolve the discrepancy. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I030  Output Interfaces:  CRA-I015 | | | |

## 5.35 CRA-F035: View / Maintain Metering System Details

| **Requirement ID:**  CRA-F035 | **Status:**  Mandatory | **Title:**  View / Maintain Metering System Details | **BSC Reference:**  CRA SD 6.4, CRA BPM 3.3, CRAWS-36, CRAWS-37, CRAWS-39 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall receive the following information about changes to the registration of the Metering Systems.   An Action Description   Authentication Details   Metering System Details (including the Meter Operator Agent for the metering system).  The CRA system shall allow the amendment of individual Metering System details;  The following validation shall be conducted:  1) That the effective from date of the change shall be no sooner than a pre-defined system wide duration [28 days] from the date of the registration request.  2) That the Meter Operator Agent specified against a metering system is registered with the CRA.  Failure of the validation rule shall be flagged to the Operator who must subsequently acknowledge that the request is valid after consultation with interested Parties. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces:  CRA-I031  Output Interfaces:  CRA-I014  CRA-I019  CRA-I022  CRA-I028 | | | |

## 5.36 CRA-F036: Maintain Flexible Reporting Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F036 | **Status:**  Mandatory | **Title:**  Maintain Flexible Reporting Requirements | **BSC Reference:**  CR 53, P8 |
| **Mechanism:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall allow an Operator to update the set of flexible reporting requests currently in force. Each request is for a BSC Party role to receive a copy of a specific report destined for another BSC Party role, for BSCCo Ltd. to receive a copy of a specific report destined for another BSC Party role or for a specific version of a report to be generated for a BSC Party.  Batches of flexible reporting requests shall be received according to interface CRA-I034.  While a copy request is in force the system shall automatically distribute a copy of the report to the requesting BSC Party (or BSCCo Ltd.). The version copied will be that generated for the original organisation.  While a version request is in force, the system shall automatically generate the requested version of the report for the requesting organisation. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input Interfaces  CRA-I034 | | | |

## 5.37 CRA-F037: Transfer from SMRS

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F037 | **Status:**  M | **Title:**  Transfer from SMRS | **BSC Reference:**  CP753 |
| **Man/Auto:**  Manual | **Frequency:**  As necessary | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| A. When a new transfer notification is initiated, CRA will receive three flows.   Meter Registration for the new metering system(s) (CRA-I031)   BM Unit Registration for the new BM Unit(s) (CRA-I005)   Transfer from SMRS details (CRA I038)  1. Process the Meter Registration according to CRA-F034, including allocation of a Metering System Identifier, but do not enter the data.  2. Send a copy of the received details (including allocated Metering System identifier) to the Transfer Coordinator.  3. Process the BM Unit registration according to CRA-F013, but do not enter the data. Send a copy of the received details to the Transfer Coordinator.  4. Check that the registrant named on the transfer initiation is a BSC Party  5. Confirm that BM Unit details have been submitted for the BM Unit(s) indicated on the transfer initiation  6. Confirm that the stated effective from date is possible  7. Confirm that the MOA in the metering systems registration is valid  8. Send a report to the transfer coordinator (CRA-I039)  B. The Transfer coordinator will subsequently submit a CRA-I038 to confirm the transfer. This flow will contain the confirmed effective from date.  1. apply the changes (as received and validated above) using the confirmed effective from date.  2. send a Transfer Summary Report (CRA-I023) to the transfer coordinator and to the new CVA registrant(s)  C. If the Transfer coordinator submits a CRA-I038 rejecting the transfer, the process is abandoned (at this stage no changes have been made).  D. If the transfer coordinator submits a CRA-I038 to confirm progress, the CRA shall respond with information regarding the progress of the transfer including completed and outstanding operations | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| The CRA shall receive notification of transfer using flow CRA-I038  The CRA shall issue transfer reports using flow CRA-I039 | | | |
| **Issues:** | | | |
|  | | | |

## 5.38 CRA-F038: Transfer to SMRS

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F038 | **Status:**  M | **Title:**  Transfer to SMRS | **BSC Reference:**  CP753 |
| **Man/Auto:**  Manual | **Frequency:** | **Volumes:** | |
| **Functional Requirement:** | | | |
| A. When a new transfer notification is initiated, CRA will receive:   Transfer to SMRS details (CRA I040)  1. Check that the Metering System is registered in CRA  2. Check that the BM Unit(s) are registered in CRA  3. Confirm that the effective to date is possible  4. Confirm that the BM Unit is ready for deregistration  5. Check whether the BM Unit is part of a Trading Unit registered using CRA-F015  6. Send a report to the transfer coordinator (CRA-I041)  B. The Transfer coordinator will subsequently submit a CRA-I040 to confirm the transfer. This flow will contain the confirmed effective from date.  1. record the effective to date  2. on receipt of deregistration requests for the Metering systems and/or BM Units, apply the changes using the confirmed effective to date  3. send a Transfer Summary Report (CRA-I023) to the transfer coordinator and to the affected PDSO  C. If the Transfer coordinator submits a CRA-I040 rejecting the transfer, the process is abandoned (at this stage no changes have been made).  D. If the transfer coordinator submits a CRA-I040 to confirm progress, the CRA shall respond with information regarding the progress of the transfer including completed and outstanding operations. | | | |
| **Non Functional Requirement:** | | | |
| If deregistrations of all Metering Systems and BM Units have not been received by 20 working days before the confirmed effective to date, then contact the registrant. | | | |
| **Interfaces:** | | | |
| The CRA shall receive notification of transfer using flow CRA-I040  The CRA shall issue transfer reports using flow CRA-I041 | | | |
| **Issues:** | | | |
|  | | | |

## 5.39 CRA-F039: Register / View / Maintain Market Index Data Provider

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F039 | **Status:**  Mandatory | **Title:**  Register / View / Maintain Market Index Data Provider | **BSC Reference:**  P78 |
| **Man/Auto:**  Manual | **Frequency:**  As Necessary | **Volumes:**  Mostly at initial set-up | |
| **Functional Requirement:** | | | |
| 1. The CRA shall allow an Operator to manually enter new Market Index Data Provider (MIDP) Registration Information into the CRA system.  The BSSC Ltd shall submit registration information to the CRA system including details of:   An Action Description to specify the type of registration operation,   the MIDP (name, contact details),  A detailed description of the interface content may be found in CRA-I042.  Where the data has passed validation the information shall be stored within the CRA system database after being authorised by a Supervisor. The CRA system shall then allocate and return to the Operator a meaningful and unique MIDP ID.  The CRA system shall also provide the MIDP with sufficient information for the authentication of future communications, electronic or otherwise. | | | |
| 2. The CRA system shall, on receipt of a new Market Index Data Provider Registration request, create a unique and meaningful party identifier.  The CRA system shall perform a check against the name of the MIDP and currently stored MIDP.  To avoid errors of duplication, should a potential duplicate MIDP name be found, the system will issue a warning which must be overridden prior to allocation of a new identifier | | | |
| 3. The CRA system shall allow an Operator to view and maintain Market Index Data Provider details.  Full details of the flow may be found in CRA-I042. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| Input interfaces:  CRA-I042  Output Interfaces:  CRA-I014 | | | |

## 5.40 CRA-F040: Provide BSCCo with Withdrawals Checklist

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F040 | **Status:**  Mandatory | **Title:**  Provide BSCCo with Withdrawals Checklist | **BSC Reference:**  CP974, P152 |
| **Man/Auto:**  Manual | **Frequency:**  On request | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall collate registration and trading details relating to a BSC Party / BSC Party Agent in response to a request for the Withdrawals Checklist received from BSCCo Ltd (via Interface Requirement CRA-I044).  1. The registration details shall be matched to the request by means of the participant id and / or participant name registered in CRA.  2. Details of BSC Party / BSC Party Agent registrations shall be provided. Where a registration has ceased to be effective, the latest Effective To date shall be provided.  3. The CRA shall obtain the trading details relating to a BSC Party by requesting information from the ECVAA (Interface Requirement CRA-I045) and the SAA (Interface Requirement CRA-I046).  4. The last day of trading for the BSC Party shall be the date of the last non-zero metered volumes held by the SAA, or the date of the last non-zero notifications held by the ECVAA, whichever is the later. Where the BSC Party has no metered volumes recorded for any settlement day then the date of the last non-zero notifications shall be used. Where the date of the last non-zero notification is "evergreen", the last day of trading for the BSC Party shall also be "evergreen".  5. The payment date of the Final Reconciliation Run for the Party's last day of trading shall be determined from the Settlement Calendar. Note that the payment date may not be known if the last day of trading is recent (within the last 14 months). | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| CRA-I044: Receive Withdrawals Checklist Request  CRA-I045: Receive Withdrawing Party Authorisation and Notification Details  CRA-I046: Receive Withdrawing Party Settlement Details  CRA-I047: Issue Withdrawals Checklist | | | |

## 5.41 CRA-F041: GC and DC Breach Monitoring

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F041 | **Status:**  Mandatory | **Title:**  GC and DC Breach Monitoring | **BSC Reference:**  P359 |
| **Man/Auto:**  Automatic | **Frequency:**  Weekly | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall monitor BM Unit Metered Volumes to identify where a BM Unit has exceeded its Generation Capacity (GC) by more than the GC Limit (a GC breach) and/or has exceeded its Demand Capacity (DC) by more than the DC Limit (a DC breach).   1. On a periodic basis (schedule to be agreed with and changed, from time to time, by BSCCo) in the current BSC Season, the CRA shall, for each BM Unit other than a Secondary BM Unit or a BM Unit undergoing a GC or DC Estimation Challenge in accordance with BSC K3.4.7J: 2. derive the GC Limits and DC Limits for each eligible BM Unit in the current BSC Season, where GC/DC Limits are set by the Panel in accordance with the Demand Capacity and Generation Capacity Limit Review and Determination document and published on the ELEXON website; 3. retrieve the BM Unit Metered Volumes (QMij) for each Settlement Day and Settlement Period in the current BSC Season (except those Metered Volumes for BMUs that occurred on Settlement Days prior to the latest effective DC in accordance with BSC K3.4.2A, i.e. a downward declaration), and ensure Metered Volumes for any Emergency Instruction (EI) that occurred during the BSC Season are subtracted from the relevant BM Unit(s) QMij; 4. determine for all eligible BM Units and every Settlement Period in the current BSC Season that has been the subject of at least the II Settlement Run if a ‘GC Breach’ and/or ‘DC Breach’ has occurred, where a GC Breach for a BM Unit is where any of its positive values of QMij (excluding any EI volumes) exceed the GC by more than the GC Limit, and a DC Breach for a BM Unit is if any negative value of QMij exceeds the DC by more than the DC Limits. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

## 5.42 CRA-F042: Identify CRA-estimated GC and DC amounts

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F042 | **Status:**  Mandatory | **Title:**  Identify CRA-estimated GC and DC amounts | **BSC Reference:**  P359 |
| **Man/Auto:**  Automatic | **Frequency:**  As required | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| This is a description of the BM Unit Volume Estimation Methodology published on the BSC Website[[6]](#footnote-7).  Where a GC Breach or a DC Breach has been identified for a BM Unit, the CRA shall, for that BM Unit, estimate a replacement QMij value (CRA-estimated GC and DC amounts) as follows, and in all cases before 1400 on the day the breach is identified:   1. Depending on whether responding to a GC breach and / or a DC breach, identify all positive QMij and/or negative QMij values for that BMU from the most recent Settlement Run for each Settlement Day and Settlement Period from the current BSC Season and the corresponding BSC Season in the previous BSC Year; 2. subtract from QMij any related Period Accepted Offer Volume(s) and/or Period Accepted Bid Volume(s) relating to Emergency Instructions that occurred on the same Settlement Day(s) and Settlement Period(s) as QMij identified in (a) above; 3. find the maximum positive QMij, which will be the CRA-estimated GC Amount; and 4. find the minimum negative QMij, which will be the CRA-estimated DC Amount. 5. Upon determining the CRA-estimated GC Amount and/or the CRA-estimated DC Amount, as applicable, the CRA will ensure the GC and/or DC for the BM Unit is updated, per CRA-F014, to reflect the CRA-estimated GC Amount and/or the CRA-estimated DC Amount. The new GC and / or DC should take effect at 00:00 on the next working day. 6. Not later than 15:00 on the day that the GC Breach or DC Breach is identified, the CRA shall notify the Lead Party of the BM Unit that the BM Unit is in GC Breach or DC Breach and will provide supporting information: 7. whether the BM Unit is in GC Breach or in DC Breach; 8. the Settlement Day and Settlement Period to which the Breach applies; 9. the relevant CRA-estimated GC or DC Amount: 10. the date on which the CRA-Estimated GC or DC Amounts will take effect[[7]](#footnote-8); 11. any other information deemed by BSCCo to be relevant; and 12. a statement to the effect that this notification will also be published on the BSC Website.     *Note that, if a BM Unit is found to be in a GC Breach and DC Breach in the same Breach Monitoring run, separate notices will be issued for the GC Breach and the DC Breach.*   1. The notice sent pursuant to 2.should also be sent to BSCCo, the CM Settlement Services Provider and the CFD Settlement Services Provider. 2. The means of communication will be agreed between the CRA and BSCCo, the CM Settlement Services Provider and the CfD Settlement Services Provider, and may change from time to time. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| CRA-Ixxx ‘Notification of a GC Breach or a DC Breach” | | | |

## 5.43 CRA-F043: Manage GC and DC Breach Challenges

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F043 | **Status:**  Mandatory | **Title:**  Manage GC or DC Estimation Challenges | **BSC Reference:**  P359 |
| **Man/Auto:**  Automatic | **Frequency:**  As required | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| 1. Where a Lead Party has been notified of a BM Unit which is in GC Breach or DC Breach, and believes that the CRA-Estimated GC or DC Amounts were calculated incorrectly (I,e. because either the CRA has not followed the BM Unit Volume Estimation Methodology correctly or the Settlement Data used is incorrect, the Lead Party may challenge the estimate(s). 2. A challenge will only be valid if submitted within 2 full Working Days of the Lead Party being notified (starting from the beginning of the Working Day following the deemed receipt of the notification); the CRA will not allow a challenge to be raised after this deadline. 3. The CRA must enable a Lead Party to submit a GC or DC Estimation Challenge online in respect of a BM Unit which is in GC Breach or DC Breach. The CRA must allow the Lead Party to provide it with the following details (the challenge details): 4. The relevant BM Unit; 5. The Settlement Date and Settlement Period relating to the GC Breach or DC Breach; 6. Evidence that the relevant positive or negative QMij was erroneous; 7. An alternative value of positive or negative QMij. 8. Where the CRA receives details of a challenge from the Lead Party, pursuant to 2 above, it shall immediately set the Appeal Status for the BM Unit to “Appealed” 9. The CRA must allow BSCCo to change the Appeal Status of any breach. 10. Where the CRA receives a GC or DC Estimation Challenge, pursuant to 2 above, it must immediately send the challenge details to BSCCo. The means of communication will be agreed, and changed from time to time, between CRA and BSCCo 11. The CRA shall receive a decision from BSCCo on a GC Breach or DC Breach Challenge within 2 full Working Days of receipt of Appeal notification, which shall include. 12. The relevant BM Unit; 13. The Settlement Date and Settlement Period relating to the GC Breach or DC Breach; and 14. Whether the decision is “Upheld” or “Rejected”; 15. For an “Upheld” decision: 16. The new value of positive QMij or negative QMij to be assigned to the BM Unit; and. 17. The Effective From Date for the new value of GC or DC. 18. Following 6 above, the CRA shall set the Appeal Status for the BM Unit to “Upheld” or “Rejected”, as appropriate, and subject to the rule set out in CRA-F044. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| CRA-IYYY “ GC Breach or a DC Breach Appeal” CRA-IZZZ ‘GC or DC Breach Appeal Decision’ | | | |

## 5.44 CRA-F044: Manage Conflicting GC/DC Submissions

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F044 | **Status:**  Mandatory | **Title:**  Manage Conflicting GC/DC Submissions | **BSC Reference:**  P359 |
| **Man/Auto:**  Manual | **Frequency:**  As required | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA may receive up to three distinct types of request to update GC and/or DC values which could have the same Effective From Date. Where the Effective From Dates are the same, the CRA shall prioritise the requests according to the order shown below, where 1 is the highest priority and 3 the lowest:   1. A value submitted by ELEXON following the conclusion of an appeal;      1. A value estimated by CRA following the identification of a breach; 2. A value submitted by the Lead Party (not as a consequence of an appeal, but in accordance with K3.4.2 and K3.4.2A).   N.b. where two or more of these requests are received with different Effective From Dates, the CRA shall process each request individually. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
| CRA-IYYY “ GC Breach or a DC Breach Appeal” CRA-IZZZ ‘GC or DC Breach Appeal Decision’ | | | |

## 5.45 CRA-F045: Publish GC and DC Breach data

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-F045 | **Status:**  Mandatory | **Title:**  Publish GC and DC Breach data | **BSC Reference:**  P359 |
| **Man/Auto:**  Automatic | **Frequency:**  As required | **Volumes:**  Low | |
| **Functional Requirement:** | | | |
| The CRA shall publish data relating to a BM Unit in GC Breach or DC Breach on the BSC Website for not less than 24 calendar months after the date of the Breach notification:   * Breach Identification Date/Time stamp * GC or DC breach * BM Unit ID * Breach SD * Breach SP * Actual BM Unit Metered Volume that triggered breach * [Prevailing] GC or DC * CRA calculated estimate of BM Unit Metered Volume * EFD for GC or DC based on CRA estimate * Appeal status – default value at the time of breach identification will be ‘No appeal’. Allowable values are: ‘No appeal’, ‘Appealed’, ‘Upheld’, ‘Rejected’ * Estimated BM Unit Metered Volume following the conclusion of an appeal (default value is NULL) * Effective From Date of the amended volume due to an appeal. When an appeal has been successfully completed the effected from date of the new GC and/or DC resulting from the appeal.   The CRA shall ensure that only the Lead Party for the relevant BM Unit will be entitled to see the above details. | | | |
| **Non Functional Requirement:** | | | |
|  | | | |
| **Interfaces:** | | | |
|  | | | |

# 6 Interface Requirements

Overview

The CRA Service shall provide an interface to the following parties.

Other Service Providers:

 Settlement Administration Agent (SAA)

 Central Data Collection Agent (CDCA)

 Balancing Mechanism Reporting Agent (BMRA)

 Energy Contract Volume Aggregation Agent (ECVAA)

 Technical Assurance Agent (TAA)

 Funds Administration Agent (FAA)

 Market Index Data Provider (MIDP)

Other external parties:

 BSC Party

 BSCCo Ltd

 System Operator (SO)

 Interconnector Administrator (IA)

 Interconnector Error Administrator (IEA)

 Supplier Meter Registration Agent (SMRA)


The CRA Service shall provide inbound and outbound interfaces as summarised in the following table. In addition to these defined flows, the CRA system (though screen printing facilities) shall be able to issue ad-hoc reports when requested to from BSCCo Ltd. These will be paper based and sent in manual form to the designated recipient.

Each interface requirement is described in detail below.

Details of the contents of interfaces relevant to the CRA are contained in the Interface Definition and Design (IDD). . In the event of discrepancies between the URS and IDD, the interface document takes precedence.

| Req. No. | Interface Requirement | I/O | Interface User | Mechanism |
| --- | --- | --- | --- | --- |
| CRA-I001 | Receive BSC Party Registration Data | I | BSC Party, BSCCo Ltd | Manual |
| CRA-I001 | Receive BSC Party Registration Data | O | BSCCo Ltd | Manual |
| CRA-I002 | Receive Interconnector Admin. Registration Data | I | BSC Party | Manual |
| CRA-I003 | Receive BSC Party Agent Data | I | BSC Party  BSCCo Ltd | Manual |
| CRA-I004 | Receive BSC Service Agent Data | I | BSCCo Ltd | Manual |
| CRA-I005 | Receive BM Unit Registration | I | BSC Party | Manual |
| CRA-I006 | Receive Trading Unit Registration | I | BSC Party | Manual |
| CRA-I007 | Receive Boundary Point and System Connection Point Data | I | BSC Party, SO | Manual |
| CRA-I007 | Receive Boundary Point and System Connection Point Data | O | BSCCo Ltd | Manual |
| CRA-I008 | Receive Interconnector Registration Details | I | SO | Manual |
| CRA-I009 | Receive BM Unit Manual Credit Qualifying Flag | I | BSCCo Ltd | Manual |
| CRA-I010 | No longer used |  |  |  |
| CRA-I011 | Receive Credit Assessment Load Factors | I | BSCCo Ltd. | Manual |
| CRA-I012 | Issue CRA Encryption Key | O | BSC Party, MIDP & other Agents | Automatic |
| CRA-I013 | Issue Authentication Details Report | O | FAA  ECVAA  BMRA  SAA  SO  BSCCo Ltd | Automatic |
| CRA-I014 | Issue Registration Report | O | BSC Party, SO & BSC Party Agents | Automatic/Manual |
| CRA-I015 | Issue BM Unit Registration Data | O | SAA,  SVAA  BMRA,  ECVAA,  FAA | Shared Database / Automatic |
| CRA-I016 | No longer used |  |  |  |
| CRA-I017 | Issue Credit Assessment Export Capability | O | SAA  ECVAA | Shared Database |
| CRA-I018 | No longer used |  |  |  |
| CRA-I019 | Issue CRA Registered Meter Data | O | CDCA | Shared Database |
| CRA-I020 | Issue Operations Registration Report | O | SO  BSCCo Ltd | Automatic |
| CRA-I021 | Issue Registered Service List | O | BSC Parties & public | Automatic |
| CRA-I022 | Issue Metering System Details | O | Technical Assurance Agent | Manual |
| CRA-I023 | Issue Registration Transfer Report | O | Transfer Coordinator,  BSC Parties,  PDSO | Manual |
| CRA-I024 | Issue Certification & accreditation Status Report | O | BSC Parties  BSC Party Agents  BSC Service Agents | Automatic/Manual |
| CRA-I025 | Receive Acknowledgement | I | All automatic outbound systems | Automatic |
| CRA-I026 | Send Acknowledgement | O | All automatic inbound systems | Automatic |
| CRA-I027 | Receive GSP Group Registration Details | I | BSC Party (Distributor) | Automatic |
| CRA-I028 | Issue NGC Standing Data Report | O | SO | Automatic |
| CRA-I029 | Receive Transmission Loss Factors | I | BSCCo Ltd | Manual |
| CRA-I030 | Receive Exception Report | I | SAA  ECVAA  BMRA | Automatic |
| CRA-I031 | Receive Metering System Data | I | BSC Party | Manual |
| CRA-I033 | Requirement not currently used |  |  |  |
| CRA-I034 | Flexible Reporting Request | I | All automatic outbound systems | Manual |
| CRA-I035 | CRA BSC Section D Charging Data | O | BSCCo Ltd | Manual |
| CRA-I036 | Send Notification Agent Termination Request | O | ECVAA | Manual |
| CRA-I037 | Receive Notification Agent Termination Feedback | I | ECVAA | Manual |
| CRA‑I038 | Transfer from SMRS information | I | Transfer Coordinator, BSC Party | Manual |
| CRA‑I039 | Transfer from SMRS report | O | Transfer Coordinator | Manual |
| CRA‑I040 | Transfer to SMRS information | I | Transfer Coordinator, BSC Party | Manual |
| CRA‑I041 | Transfer to SMRS report | O | Transfer Coordinator | Manual |
| CRA-I042 | Receive Market Index Data Provider Registration Data | I | BSCCo Ltd | Manual |
| CRA-I043 | Receive Exempt Export Registration Data | I | BSCCo Ltd | Manual |
| CRA-I044 | Receive Withdrawals Checklist Request | I | BSCCo Ltd | Manual |
| CRA-I045 | Receive Withdrawing Party Authorisation and Notification Details | I | ECVAA | Manual |
| CRA-I046 | Receive Withdrawing Party Settlement Details | I | SAA | Shared Database |
| CRA-I047 | Issue Withdrawals Checklist | O | BSCCo Ltd | Manual |

The following diagrams illustrate these interface requirements.



**CRA Service: Inbound Interface Requirements**



**CRA Service: Outbound Interface Requirements[[8]](#footnote-9)**

# 7 Non Functional Requirements

This section specifies non-functional requirements of the CRA Service.

## 7.1 CRA-N001: Input Interface Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-N001 | **Status:**  M | **Title:**  Input Interface Requirements | **BSC Reference:**  CRAWS-40, CN122 |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  Low | |
| **Non Functional Requirement:** | | | |
| 1. The CRA system shall provide manual input mechanisms for the insertion of data into the system from external parties where stated.  2. The CRA service shall provide a mechanism for the decoding of electronically transferred data so that an operator may enter the details contained in the messages.  3. The CRA service shall provide functionality for a user to select an electronic data notification from a list of outstanding input messages and display the contents in a human readable form. Data items shall be listed alongside a label describing individual fields in the input data flow.  4. The CRA system shall allow an Operator to ‘cut and paste’ the information in these messages into the relevant input screens.  5. The CRA service shall carry out validation of all data input so as to ensure that the data is, as far as is practicable, complete and consistent.  6. Where data is to be input manually, the service shall use reasonable endeavours to ensure that the quality of the data is not compromised in any way. The exact mechanism to ensure this is conducted will be developed in detail within the System and Detailed Design Specification.  7. All registration actions or changes to registered data shall require the prior approval of BSCCo Ltd. This is expected to be in the form of paper based supporting documentation. An Operator shall be expected to check that this authorisation has been received when processing the Registration request and facilities (tick-boxes, document reference fields) will be available on the input forms to:   allow for cross-referencing between paper and electronic registration information   log that this check has been completed  8. Should the data, once entered on the input form pass input validation but require confirmation from either a second Party or BSCCo Ltd, the Operator shall then be presented with the ability to save the valid parts of the registration (subject to database constraints) in a “Pending” state rather than having to abort the entire update. While in this state, the data will be “invisible” to other parts of the BSC Central Systems. For instance it will not be issued to other Services (CDCA, SAA). At a later time, the Operator shall be able to retrieve the partial update and complete when the original failure has been corrected.  9. Certain registration items (such as BM Units) are expected to be registered from a limited sub-set of Party types. The CRA system shall ensure that a check against Party type is conducted on entry or amendment of registration details. However, where an unexpected registration request is detected, the CRA shall not fail the operation outright. Rather, the Operator shall be required to override the failure explicitly.  10. When overriding a “Warning” from either point 8 and 9 above, it may be necessary that the level of authority for the override operation be increased from an Operator. A Supervisor may, in some cases, be required to clear a specific Warning type. These roles shall be described in more detail in the CRA System Specification.  11. All registration entries / amendments will be tagged with the date and time of the operation as well as the identifier (username) of the Operator who entered the details. In addition, where a validation Warning is expressly overridden, the Operator / Supervisor’s identification will also be logged.  12. Each registration operation may require a specific level of authorisation within the requesting Party. The CRA stores these levels of authorisation and shall validate that the requesting person has the authorisation to conduct the requested operation. Where this check fails the CRA shall reject the entire request.  13. The CRA system shall (with exceptions such as on change of ownership of BM Units and Interconnector Error Administration responsibility) only accept registration amendments from the Party that sent in the original registration request.  14. The CRA Service shall undertake Interface Tests for all Parties wishing to register within the CRA. The interface tests will cover the following services (as appropriate to the applicant):   BMRA;   CDCA;   CRA;   FAA and   SAA.  15. Where Validation errors occur within the system as either a result of individual data entry or through the daily validation check (CRA-F023) the system shall allow the failures to be viewed and searched for by an Operator in accordance with the following:   The system shall present each validation warning / failure to the Operator through an online screen on demand for subsequent rectification through View / Maintain functionality described in previous appropriate requirements in Section 5.   The CRA system shall allow an Operator to search through the highlighted information by failure type, BSC Party and effective to / from dates to limit the amount of information presented at any one time. | | | |

# 8 Service Requirements

This section details the Service Requirements for the CRA system. General requirements can be found in Appendix E

## 8.1 CRA-S001: Message Security and Encryption

| **Requirement ID:**  CRA-S001 | **Status:**  Mandatory | **Title:**  Message Security and Encryption | **BSC Reference:**  CRAWS-55 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  Low | |
| Non **Functional Requirement:** | | | |
| The CRA system shall receive electronic data in either encrypted or non-encrypted format. Each Party may exchange data with the CRA system using one or more encryption public keys. BSC Party information shall always be received using a notified encryption key, whereas Service Agents shall not be required to use encryption.  The CRA system shall communicate back to Parties using the encryption public key supplied from the party where supplied and the use mandated. | | | |

## 8.2 CRA-S002: Data Migration Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  CRA-S002 | **Status:**  Mandatory | **Title:**  Data Migration Requirements | **BSC Reference:**  CR990813\_07, CRAWS-56 |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:** | |
| Non **Functional Requirement:** | | | |
| Detailed Data Migration requirements will be established during the detailed design phase. | | | |
| **Issues:** | | | |
| Data Migration requirements need to be discussed with the Customer in detail and will be documented separately outside of the scope of the URS. | | | |

## 8.3 CRA-S003: Archiving Requirements

| **Requirement ID:**  CRA-S003 | **Status:**  M | **Title:**  Archiving Requirements | **BSC Reference:** |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:** | |
| Non **Functional Requirement:** | | | |
| The CRA shall provide a suitably secure repository for any documents or paper based information provided by BSC Parties in connection with their Registration or generated by the CRA in connection with the operation of their registration service.  This requirement is in addition to all general archiving requirements as stated in GEN-S004. | | | |
| **Issues:** | | | |
|  | | | |

# 9 User Roles and Activities

The following table describes the user roles which will support the day to day operation of the CRA service.

| Role | Activities |
| --- | --- |
| System Administrator | Database management  Specific aspects of system configuration  User account and security management |
| Supervisor | Management of Operators  Management of standing data updates  Management of planned operational and service level requirements  Creation of management information reports  Support for communication with external parties |
| Operator | Performance of procedures to monitor receipt and processing of information from external parties.  Second level support for ad hoc queries raised by external parties |
| Help Desk Operator | First level support for ad hoc queries raised by external parties. |
| Auditor | There shall be a specific user security configuration which allows an external auditor to review data within the system, but prevents the initiation of batch processes or logical edits to business data. |
| Market Index Data Provider | Market Index Data Providers are registered by BSCCo Ltd, and their details are passed on by CRA to SAA and BMRA. |

The following parties are defined as users of the service. The detailed functional requirements and data interfaces necessary to support these parties are described earlier in section 6 of this URS.

|  |  |
| --- | --- |
| Role | Summary of Activities related to CRA |
| BSCCo Ltd. | Receives summary settlement reports from CRA at periodic intervals (daily, weekly, monthly) as well as CRA performance reports. |
| Balancing Mechanism Operator (NGET ) | Reports are produced to NGET on Standing data held within the system. |
| BSC Party | BSC Parties register information (such as their own registration) as well as registration details of BM Units, Trading Units, etc. They also receive confirmation that these registrations have been either successful applied or failed for some reason. |
| SAA | The SAA is sent authentication and registration details by the CRA. In addition, the CRA informs the ECVAA of the WDBMCAIC and NWDBMCAIC. |
| ECVAA | The ECVAA is sent authentication and registration details by the CRA. . |
| CDCA | The CDCA is sent authentication and registration details by the CRA.. |
| SMRA | The SMRA is sent details of the Boundary Points registered within the CRA system. The CRA also receives back a subset of this list if they are registered within the SMRA. |
| Interconnector Administrator | The Interconnector Administrator arbitrates when a change of Interconnector Error Administrator event occurs. |
| Funds Administration Agent (FAA) | The FAA is sent registration details by the CRA. |
| Public | The Public are entitled to view the list of Registered Service Providers. |
| TAA | The TAA is sent a list of the registered Boundary Points and Metering Systems. |

# 10 Future enhancements

No future enhancements to the CRA service have been identified at this stage.

Please refer to Appendix F for common future requirements.

**Appendix A Requirements Compliance Matrix**

The following table shows the mapping of requirements defined in this URS document to the requirements set out in the Service Description for Central Registration [CRA SD].

| Service Description Requirement Number or CR Number | URS Requirement Reference Number | Notes |
| --- | --- | --- |
| 4.1.1 | CRA-F001  CRA-F002  CRA-F006  CRA-I001 |  |
| 4.1.2 | CRA-F004  CRA-F005  CRA-I014 |  |
| 4.1.3 | CRA-F007  CRA-F008  CRA-I002  CRA-I014 |  |
| 4.1.4 | CRA-F001  CRA-F006 |  |
| 4.1.5 | GEN-S003 |  |
| 4.1.6 | CRA-F002  CRA-F003  CRA-I001 |  |
| 4.1.7 | CRA-F002  CRA-F003  CRA-I001  CRA-I011 |  |
| 4.2.1 | CRA-F009  CRA-F010  CRA-I003 |  |
| 4.2.2 | CRA-F009  CRA-F010  CRA-I003 |  |
| 4.3.1 | CRA-F011  CRA-F012  CRA-I004 |  |
| 4.3.2 | CRA-F011  CRA-F012  CRA-I004 |  |
| 5.1 | CRA-F011  CRA-F012 |  |
| 5.2 | CRA-F011 |  |
| 5.3 | CRA-I021  CRA-I024 |  |
| 6.1.1 | CRA-F013  CRA-F014  CRA-I005 |  |
| 6.1.2 | CRA-F013 |  |
| 6.2.1 | CRA-F015  CRA-F016  CRA-I006 |  |
| 6.2.2 | CRA-F015 |  |
| 6.2.3 | CRA-F015  CRA-F016 |  |
| 6.3.1 | CRA-F019 |  |
| 6.4.1 | CRA-F017  CRA-F018  CRA-I007 |  |
| 6.4.2 | CRA-F017  CRA-F018  CRA-I007 |  |
| 7.1.1 |  | BMCAIC now calculated in CRA |
| 7.1.2 | CRA-I017 |  |
| 7.2.1 | CRA-F013  CRA-F014  CRA-F022  CRA-I017 |  |
| 7.2.2 | CRA-F020  CRA-I011  CRA-I017 |  |
| 8.1 | CRA-F023 | Validation rules may be found in all requirements as well as the central validation check. |
| 9.1 | CRA-I014 |  |
| 9.2 | GEN-N002 |  |
| 9.3 | GEN-N002  GEN-N003  GEN-S004 |  |
| 10.1 | CRA-I014 |  |
| 10.2 | CRA-I014 |  |
| 10.3 | CRA-I022 |  |
| 10.4 | CRA-I013 |  |
| 10.5 | CRA-I015 |  |
| 10.6 | CRA-I013 |  |
| 11.1 | CRA-I019 |  |
| 11.2 | CRA-I023 |  |
| 11.3 | CRA-I015 | Due to the nature of the shared database, the CDCA would not need to request a refresh since the data is always up to date |
| 12 | GEN-S006 |  |
|  |  |  |
| CR 53 | CRA-F036  CRA-I034 |  |
| CR 65 | CRA-I035 |  |
| CP503 | CRA-F010  CRA-I036  CRA-I037 |  |
| CP508 | CRA-F006  CRA-I001 |  |
| CP569 | CRA-F034  CRA-I031 |  |
| P8 | CRA-F036  CRA-I034 |  |
| CP753/P55 | CRA-F013  CRA-F034  CRA-F025  CRA-F037  CRA-F038  CRA-I005  CRA-I031  CRA-I023  CRA-I038  CRA-I039  CRA-I040  CRA-I041 |  |
| P78 | CRA-F039  CRA-I012  CRA-I013  CRA-I014  CRA-I042 |  |
| CP975 | CRA-I013 |  |
| CP974 | CRA-F040  CRA-I044  CRA-I045  CRA-I046  CRA-I047 |  |
| P197 | CRA-F001  CRA-F009  CRA-F010  CRA-F011  CRA-F025  CRA-F027  CRA-I003  CRA-I019  CRA-I021  CRA-I024 |  |
| CP1193 | CRA-F002  CRA-I013 |  |
| P215 | CRA-F013  CRA-F014  CRA-I009  CRA-I014  CRA-I015  CRA-I020 |  |
| P268 | CRA-F013  CRA-F014 |  |
| P269 | CRA-F013  CRA-F014 |  |
| P310 | CRA-F020  CRA-F022  CRA-F027  CRA-I014  CRA-I020  CRA-I011 |  |
| P359 | CRA-F041  CRA-F042  CRA-F043  CRA-F044 |  |

**Appendix B Logical Data Model**

The Logical Data Model is maintained separately by BSCCo and is available on request.

**Appendix C Business Process Model**

Below is reprinted the business process model as provided within the CRA BPM. The requirements in this document, in places map directly to process blocks within the BPM. In other cases, and specifically where a requirement has been found within the SD and not mentioned within the BPM, additional processes have been created. As such, the model is provided for reference and information only, though all requirements in the main section of the document supersede the processes below.



**Appendix D NETA Central Service Common Non Functional Requirements**

This section details the non-functional requirements common to the entire suite of User Requirements Specifications. Only common requirements are detailed within this section - e.g. where a requirement is specific to a given sub-system it is detailed within the individual URS only.

D-1 GEN-N001: Audit Requirements

| **Requirement ID:**  GEN-N001 | **Status:**  M | **Title:**  Audit Requirements | **BSC Reference:**  Schedule 3 Part B |
| --- | --- | --- | --- |
| **Man/Auto:**  Automatic | **Frequency:**  All business transactions (including manual filing) | **Volumes:**  Audit information shall be associated with each set of data created by any business transaction. Volumes will be established during detailed design. | |
| **Non Functional Requirement:** | | | |
| 1. All business data received by the Service Provider from external sources shall be retained and not physically deleted, subject to the retention durations described in GEN-S004. Multiple versions of the data shall be supported, for instance so that both the original information and any subsequent corrections are separately stored. Business data shall have an associated effectiveness date range which identifies the trading dates to which it is applicable.  2. The Service Provider shall maintain an audit trail of when information from external sources was received, from whom, and when the information was processed.  3. All business data transmitted to external parties by the Service Provider shall be retained and not deleted, subject to the retention durations described in this document. Multiple versions of the data shall be supported, for instance so that the results of settlement calculations in successive settlement runs for the same trading day are available individually.  4. Any changes made to business data by operators of the service shall be retained as a new data version, i.e. data may only be ‘logically’ modified, not physically modified thus retaining a copy of the previously un-modified business data. It shall not be possible for Operators to physically delete business data, though it shall be possible to ‘logically’ delete data such that it is not included within any subsequent computation or reporting process. Any business data which is entered, logically modified or logically deleted by Operators of the service shall be time stamped to record the time the transaction occurred, and the identity of the Operator who performed the transaction shall be recorded. This audit information shall be available for inspection by a suitably authorised party.  5. The Service Provider shall ensure that all output files and reports produced are uniquely identifiable and time stamped.  6. The Service Provider shall arrange for all printed reports that are no longer required for the provision of Services or for audit to be securely destroyed.  7. The Service Provider shall arrange for the removal from machine-readable media and subsequent secure destruction of all data that is no longer required.  8. The Service Provider shall facilitate the following specific requirements of the BSCCo Ltd appointed Auditor. The Service Provider shall facilitate any reasonable audit requirements to ensure:   The Service is being run in accordance with BSC rules.   Validation of Service providers’ performance (service credits, etc.)   Any modification to the Service is carried out in accordance with the BSC modifications rules. | | | |

D-2 GEN-N002: Security Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  GEN-N002 | **Status:**  M | **Title:**  Security Requirements | **BSC Reference:**  Schedule 3 Part B Section 4 |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  N/A | |
| **Non Functional Requirement:**    The Service security procedures shall be created in accordance with BS7799. These procedures will be fully defined in the Operational Services Manual.  Procedures are likely to include the following. | | | |
| 1. All buildings used by the Service Provider in connection with provision of the service shall be made secure in that only suitably authorised persons may obtain entry. This shall include the use of keycard, numeric keypad or other physical barriers which prevent casual entry to the premises. Visitors to the premises shall undergo a procedure which ensures that their entry to the premises is suitably authorised and their access to the parts of the site controlled thereafter. Both the normal and disaster recovery sites shall have sufficient provision to ensure that the security of the buildings is not compromised outside standard working hours.  2. Key elements of the infrastructure used to support the service such as computer server hardware, power supplies and other essential physical equipment shall be subject to further physical restrictions such that they are only accessible to suitably authorised personnel, and not to other operational staff or visitors. Such hardware shall be protected by specialist mechanisms such as a gas flooding capability in order to reduce the impact on the service of accidents such as fire or flooding.  3. The bespoke computer applications used to support the service shall be subject to entry of a secure username and non-displayed password before access to any data or function relevant to the service is possible by an operator. Passwords will be updated through procedural means on a regular basis, users shall be forced to change passwords on a periodic cycle (maximum of 2/3 months). Users shall also be prevented from using easily guessed passwords and refused the reuse of their most recently used passwords.  4. The bespoke systems supporting the service shall be configurable such that individual functions are available only to authorised categories of user. It shall be possible furthermore to configure the systems such that a user interface function which accesses business data can be made available only in a read-only mode to those categories of user with restricted security privileges. Categories of user with higher levels of security privilege shall be able to enter, logically modify and logically delete data using the same facilities. If a user has read access to a function, they may review all data accessible using that function.  5. The Service Provider shall monitor any attempts to breach the physical and logical security of the System and report any such occurrences to the Customer. When any such attempt is discovered, the Service Provider shall use all reasonable endeavours to identify the cause of the breach and to ascertain whether the existing controls are adequate.  6. All user workstations should provide a password controlled screen time out facility. This may be provided through the use of standard facilities included in the workstation operating system, or other commercially available tools.  7. The Service Provider shall use a secure communications infrastructure for transfer of data to another person / system and for receipt of data from the System Operator and other Parties. The infrastructure must support the following:   authentication: a mechanism to verify that the parties on either side of the data link are who they claim to be;   privacy: a mechanism to ensure that transmitted content is not read or intercepted by unauthorised recipients;   integrity: a mechanism to verify that transmitted data is received in an unchanged state. | | | |

D-3 GEN-N003: Operational Control

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  GEN-N003 | **Status:**  M | **Title:**  Operational Control | **BSC Reference:**  Service Agreement Schedules |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:** | |
| **Non Functional Requirement:**    The operational procedures will be fully defined in the Operational Services Manual.  Procedures are likely to include the following. | | | |
| 1. It shall be possible for Operators of the service to have control over the loading of data files from external parties. This will include the ability to turn on and off file loading selectively, based on file type and sender.  2. The contents of an inbound data file shall be viewable by an Operator either before or after the file has been loaded into the system.  3. In the event of data loading errors caused by problems with standing data (e.g. registration data) it shall be possible to re-load the information once these errors have been corrected (e.g. after consultation with the CRA Service Provider).  4. The systems supporting the service shall be configurable such that the recipients of each type of individual report process can be defined.  5. It shall be possible to configure the system such that reports are either automatically scheduled for release to their recipient destinations, or else are released only by specific intervention of an Operator.  6. Any report file shall be inspectable by a suitably privileged Operator either before or after it has been made available to its recipient.  7. It shall be possible to cause individual batch and report processes to be initiated either on demand, at a pre-scheduled date and time, or to repeat automatically at a periodic interval.  8. It shall be possible for an Operator to monitor the progress of any individual batch or report process, for instance to review any informational or warning logs generated so far by the running process.  9. It shall be possible for Operators to cancel any scheduled batch or report process, or kill any individual process while it is running, such that updates to the business data are rolled back and not committed.  10. The initiation of a batch or report process shall not prevent Operators from performing other tasks within the system using the same workstation, i.e. they are not required to wait for the batch or report process to complete before they can proceed to use other system functions.  11. It shall be possible to configure the system such that individual batch or report processes run automatically as a result of successful completion of other automated tasks. For instance, the successful completion of one batch process could automatically trigger a report based on data created by that batch process.  12. Reports containing data shall be made available in a machine readable format, with individual data fields separated by a delimiter character, and numeric fields being represented in a specified format, including the explicit use of decimal points where required. A definition of a standard physical file convention shall be established in the Design Phase as part of the Interface Definition and Design Specification, and be made available to BSCCo Ltd for distribution to relevant parties.  13. Suitably authorised Operators of the system shall be able to obtain printed copies of any report.  14. Operators of the system shall be able to obtain printed copies of any data which they are able to display via the user interface, given their security privileges. This includes snapshots of the current status of system management monitoring functions to which they have access, and a print of business data which they may have selected via a query on a data maintenance screen.  15. Operators of the system shall be able to save to a text file copies of any business data which they may have selected via a query on a data maintenance screen, given their security privileges. This text file should include the data in a simple comma-separated format compatible with standard desktop tools such as spreadsheets and word processors. | | | |

D-4 GEN-N004: Euro Compliance

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  GEN-N004 | **Status:**  Mandatory | **Title:**  Euro Compliance | **BSC Reference:**  PPR- Action 3.2 |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  N/A | |
| **Non Functional Requirement:** | | | |
| The Trading Arrangements on Day 1 of Trading shall be in Sterling and Trading in Euros shall not be permitted.  The NETA system and services shall not preclude being Euro Compliant in accordance with legal requirements applicable in England at a later date and after “Euro Compliancy” is further defined.  Also refer to Appendix F - Common Future Requirements. | | | |

D-5 GEN-N005: Help Desk Queries

| **Requirement ID:**  GEN-N005 | **Status:**  Mandatory | **Title:**  Help Desk Queries | **BSC Reference:**  Schedule 3 part 2 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As required | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The system shall respond to queries within the timescales set out below:  1. For FAX and e-mail queries, the Operator shall register the query into the system within 15 minutes of receipt.  2. For Postal queries, the Operator shall register the query into the system within 4 hours of receipt.  3. For telephone queries, the Operator shall register the query immediately.  4. The system shall provide a 24hr help-desk facility.  The system shall allocate an appropriate severity level and respond to the query within the following timescales at a service level of greater than 95%. | | | |

| Type of Incident | Severity Level | 1st Call Back to caller | Follow-up Calls to caller | Escalation to the Customer |
| --- | --- | --- | --- | --- |
| Immediate or sustained threat to the settlement timetable and output to Funds Administrator. | 1 | 10 minutes | every 20 minutes | 1 hour elapsed |
| Potential impact on settlement timetable or major problems for Participants with reports. | 2 | 10 minutes | every 20 minutes | 4 working hours |
| Severe impact on the accuracy of settlement data. | 3 | 30 minutes | every 1 hour | 8 working hours |
| Minor data error. | 4 | 4 hours | every 8 hours | 2 working days |
| General enquiries. | 5 | 24 hours | every 24 hours | 7 elapsed days |

|  |
| --- |
| Reports against the service level requirements shall be produced as per URS specific Reporting functionality. |

D-6 GEN-N006: Help Desk SLA Reporting

| **Requirement ID:**  GEN-N006 | **Status:**  Mandatory | **Title:**  Help Desk SLA Reporting | **BSC Reference:**  ITT Schedule 2 2.8 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As required | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The Services shall produce reports monthly detailing the level of service provided by the agency to the BSCCo Ltd. The reports shall detail the response times in delivering various aspects of the system as detailed below. The Service level for each of the activities is contained within the braces in each case.  1) Register fax and e-mail queries into system within 15 minutes of receipt (100%)  2) Register postal query into system within 4 hours of receipt (100%)  3) Register telephone query immediately upon receipt (100%)  4) Query calls allocated an appropriate severity level and responded to within the timescales prescribed in GEN-N004. (95%)  5) Reports produced detailing Problems logged by Severity Level, total calls, calls answered in 10 seconds, confirmation of calls within response time, call sign off date outstanding problems that are outside the time-scale. (100%)  6) First reply to user in time-scale by Severity Level, second reply to user in time-scale by Severity Level, third reply to user in time-scale by Severity Level, subsequent replies to user in time-scale by Severity Level; (95% of calls for each severity level responded to within prescribed timescales)  7) Totals of problems solved within the agreed response times, those calls escalated and any outside the time-scales  8) Summary of all outstanding problems and their status including a copy of the current Help Desk Service Log | | | |

D-7 GEN-N007: Input Interface Requirements

| **Requirement ID:**  GEN-N007 | **Status:**  Mandatory | **Title:**  Input Interface Requirements | **BSC Reference:** |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  As required | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The Services shall carry out validation of all data input so as to ensure that the data is, as far as is practicable, complete and consistent.  Where data is to be input manually, the service shall use reasonable endeavours to ensure that the quality of the data is not compromised in any way. Data will be input in line with agreed service level agreements. The exact mechanism to ensure this is conducted will be developed in detail within the System and Detailed Design Specification. | | | |

**Appendix E NETA Central Services Common Service Requirements**

This section details the Service Requirements common to the entire suite of User Requirements Specifications. Only common requirements are detailed within this section - e.g. where a requirement is specific to a given sub-system it is detailed within the individual URS only.

E-1 GEN-S001: Volumetric Requirements

| **Requirement ID:**  GEN-S001 | **Status:**  M | **Title:**  Volumetric Requirements | **BSC Reference:**  Schedule 4 Part C Section 4  RETA ITT: A3 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  As below. | |
| **Non Functional Requirement:** | | | |
| The following tables give indicative volumetric details and are for information only. | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| Assumption |  | Volumes |  |
|  | Low | Average | High |
| BM Units |  | 1,000 | 5,000 |
| BSC Parties | 100 | 200 | 300 |
| Settlement Periods | 46 | 48 | 50 |
| Energy Accounts per BSC Party | 2 | 2 | 2 |
| Metering Systems | 4,000 | 5,000 | 10,000 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Transaction | Explanation |  | Volumes |  |
|  |  | Low | Average | High |
| Aggregated Debits/Credits per day | BSC Service User \*  5 Settlement Runs \*  1 Settlement Day | 500 | 1,000 | 1,500 |
|  | (3 after Bank Holidays, etc.) | (1,500) | (3,000) | (4,500) |
| Disputes resolved per week | Expected number of disputes | 10 | 30 | 50 |
| Reports produced per day | Assumed 5-20-45 Reports per BSC Service User per day | 500 | 4,000 | 13,500 |

E-2 GEN-S002: Resilience and Availability Requirements

| **Requirement ID:**  GEN-S002 | **Status:**  M | **Title:**  Resilience and Availability Requirements | **BSC Reference:**  Schedule 4 Part C Section 1 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| Software and Data must be allocated over the Hardware configuration such as to ensure that agreed service levels are met.  The Service Provider shall ensure that no more than one day’s on-line Data is lost as a result of any failure of the System or Services. Any known lost Data will be recreated.  The Service Provider shall ensure that there is no permanent loss of Data. | | | |

E-3 GEN-S003: Backup and Recovery Requirements

| **Requirement ID:**  GEN-S003 | **Status:**  M | **Title:**  Backup and Recovery Requirements | **BSC Reference:**  Schedule 3 Part B Section 5 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As below. | **Volumes:**  As below. | |
| **Non Functional Requirement:** | | | |
| 1. The Service Provider shall run, and record successful completion of, daily backup procedures for all on-line databases and maintain a documented backup log. The Customer shall be entitled to check on a random basis that all back-ups are completed and that a backup log is being maintained.  2. The Service Provider shall identify each backup and ensure that all backups are held on appropriate media, labelled accurately and clearly.  3. The Service Provider shall ensure that all backups are secured in two locations (one off-site) in fire proof and flood proof, safe environments, appropriate to the type of backup, as recommended by the media manufacturer.  4. The Service Provider shall ensure that backup and recovery procedures do not prejudice scheduled operations and are timed to minimise the risks of loss of data.  5. The Service Provider shall ensure that back up recovery times are compatible with service availability requirements.  6. The Service Provider shall ensure that all Data and Software necessary to support the Services are backed up at regular intervals in accordance with the timetable and procedure set out in the Operational Services Manual.  7. The Service Provider shall, at regular intervals not exceeding three months, ensure that the backup files could be restored if required. | | | |

E-4 GEN-S004: Archiving Requirements

| **Requirement ID:**  GEN-S004 | **Status:**  M | **Title:**  Archiving Requirements | **BSC Reference:**  Schedule 3 Part B Section 6 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  As below. | |
| **Non Functional Requirement:** | | | |
| 1. The Service Provider shall identify each archive and ensure that all archives are held on appropriate media, labelled accurately and clearly, in line with media manufacturer’s recommendations. All items should contain their original creation (or received) date and the date of archive.  2. The Service Provider shall ensure that all archives are secured in one or more offsite locations in fire proof and flood proof, safe environments, appropriate to the type of archive media, as recommended by the media manufacturer.  3. The Service Provider shall ensure that all archived material is retained and retrievable, in accordance with the following (unless specified otherwise in the individual URSs):   on-line access must be available within 5 minutes for Data up to one month old;   on-line access must be available within 24 hours for Data up to one year old;   on-line access must be available within one week for Data up to seven years old.  4. The specific user identified archive requirements shall be detailed within the individual URS and System Specifications.  5. A document proposing archive strategy for the database shall be provided once the physical data model has been constructed and archive requirements for the URS’s have been agreed. | | | |
| **Issues:** | | | |
| Full archiving requirements will be detailed outside the scope of this document. | | | |

E-5 GEN-S005: Synchronise System Time

| **Requirement ID:**  GEN-S005 | **Status:**  Mandatory | **Title:**  Synchronise System Time | **BSC Reference:**  CRA SD 12 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  Daily | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The Service Provider shall ensure its systems are set in accordance with the Universal Time Clock (UTC), adjusting the time as necessary, at least once every 24 hours. | | | |

E-6 GEN-S006: Query Resolution

| **Requirement ID:**  GEN-S006 | **Status:**  Mandatory | **Title:**  Query Resolution | **BSC Reference:**  CRA Appendix B |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual | **Frequency:**  Daily | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The Services shall provide facilities for the logging of queries from external agencies. The Service shall allow an Operator to enter details of the query into the system including the date / time of query incidence, the originating person / system, contact name (where appropriate) and the nature of the query.  Each query shall be assigned a severity level on the basis of the nature of the query in accordance with the requirements of GEN-N005. The severity level may be subsequently changed only be suitably authorised personnel.  The system shall require authentication details to be received prior to query functionality where mandated by the nature of the query.  The system shall log details of the query and return a unique query reference number to the originating party.  The system shall allow a query to be progressed through a number of states, depending upon the nature of the query, through to resolution. At each stage in this process, the actions of the Operator in advancing the query shall be logged against the user ID and date of time of advancement. Queries may only be ‘signed off’ by suitably authorised personnel.  Details of all queries entered into the system shall be maintained within the system subsequent to sign off.  The system shall provide reporting facilities on the range and resolution of problems:  1) Daily, A report shall be produced detailing Problems logged by Severity Level, total calls, calls answered in 10 seconds, confirmation of calls within response time, call sign off date.  2) Daily, a summary of all outstanding problems and their status | | | |
| **Issues:** | | | |
| A number of the service levels do not currently have an agreed timescales against which the service level percentage shall be judged. These shall be considered during the detailed design | | | |

E-7 GEN-S007: Performance Requirements

| **Requirement ID:**  GEN-S007 | **Status:**  Mandatory | **Title:**  Performance Requirements | **BSC Reference:**  Schedule 4 Part C Section 3 |
| --- | --- | --- | --- |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  Daily | **Volumes:** | |
| **Non Functional Requirement:** | | | |
| The Service Provider shall ensure that during Normal Operation,   on-line access is achieved in accordance with agreed service levels   all batch processes execute in time to meet agreed service levels  Normal Operation includes any commonly predictable periods of peak transaction rates.  Relevant service level agreements will be detailed outside the scope of this document. | | | |
| **Issues:** | | | |
|  | | | |

E-8 GEN-S008: Data Retention Requirements

| **Requirement ID:**  GEN-S008 | **Status:**  Mandatory | **Title:**  Data Retention Requirements | **BSC Reference:**  P107 |
| --- | --- | --- | --- |
| **Man/Auto:**  Automatic | **Frequency:**  Ongoing | **Volumes:**  N/A | |
| **Non Functional Requirement:** | | | |
| The CRA, CDCA, SAA and ECVAA shall retain a minimum of 40 months of Settlement Data to support the Trading Disputes process. The latest 28 months of Settlement Data shall be retained on-line such that Settlement Runs or Volume Allocation Runs can be supported. A further 12 months Settlement Data shall be retained such that queries can be made to support Extra‑Settlement Determinations. | | | |
| **Issues:** | | | |
|  | | | |

**Appendix F NETA Central Services Common Future Requirements**

F-1 GEN-EURO: Euro Compliance

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID:**  GEN-EURO | **Status:**  Mandatory | **Title:**  Euro Compliance | **BSC Reference:**  PPR- Action 3.2 |
| **Man/Auto:**  Manual & Automatic | **Frequency:**  As required | **Volumes:**  N/A | |
| **Functional Requirement:** | | | |
| The Service Provider Hardware, Software and System will operate using financial data expressed in both the original currency and euros.  Appropriate modifications will be made in the data structure and relevant software programs and interfaces in order to accommodate the above requirement. This will include, but will not be limited to, the following:  – Systems analysis.  – Data conversion and changes to the data structure.  – Changes to the relevant interfaces.  – Modification of the relevant data validation engines.  – Reception, processing and presentation of original currency and euros.  – Testing, trialling and implementation.  The ability of the Hardware, Software and System to meet the agreed Service Levels will not be impaired by the above changes. | | | |

**Appendix G Glossary**

G-1 Glossary of acronyms:

|  |  |
| --- | --- |
| WDBMCAECi MW | Working Day BM Unit Credit Assessment Export Capability |
| NWDBMCAECi MW | Non-Working Day BM Unit Credit Assessment Export Capability |
| WDBMCAICi MW | Working Day BM Unit Credit Assessment Import Capability |
| NWDBMCAICi MW | Non-Working Day BM Unit Credit Assessment Import Capability |
| BOLRnij(t) MW | Bid-Offer Lower Range |
| BOURnij(t) MW | Bid-Offer Upper Range |
| BSAPmj | Balancing Services Adjustment Price |
| CABknij £ | Period Acceptance Bid Cashflow |
| CAEIaj £ | Account Energy Imbalance Cashflow |
| WDCALFi | Working Day Credit Assessment Load Factor |
| NWDCALFi | Non-Working Day Credit Assessment Load Factor |
| CAOknij £ | Period Acceptance Offer Cashflow |
| CAOknij £ | Period Acceptance Offer Cashflow |
| CAPP (£/MWh) | Credit Assessment Purchase Price |
| CASP (£/MWh) | Credit Assessment Sale Price |
| CBMij £ | Period BM Unit Cashflow |
| CBnij £ | Period BM Unit Bid Cashflow |
| CEPaij % | Credited Energy Percentage |
| CIIij £ | Information Imbalance Charge |
| CNDBnij £ | Non-Delivered Bid Charge |
| CNDij £ | BM Unit Period Non-Delivery Charge |
| CNDOnij £ | Non-Delivered Offer Charge |
| COnij £ | Period BM Unit Offer Cashflow |
| CSOBMj £ | System Operator BM Charge |
| d | Settlement Day |
| ECQzabj MWh | Energy Contract Volume Notification Data |
| f | Point Value |
| FPNij MWh | Period FPN |
| FPNij(t) MW | Final Physical Notification |
| fFPNijt MW | Point FPN |
| g | Ramp Rate |
| GC | Generation Capacity |
| i | BM Unit |
| IIPj £/MWh | Information Imbalance Price |
| j | Settlement Period |
| k | Bid-Offer Acceptance |
| m | Balancing Services Adjustment Action |
| MDPi Minutes | Maximum Delivery Period |
| MDVi MW | Maximum Delivery Volume |
| MEL i(t) MW | Maximum Export Limit |
| fMEL it MW | Point Maximum Export Limit |
| fMIL it MW | Point Maximum Import Limit |
| MIL ij(t) MW | Maximum Import Limit |
| MNZTi Minutes | Minimum Non-Zero Time |
| MPj | Market Price |
| MZTi Minutes | Minimum Zero Time |
| n | Bid |
| NDZi Minutes | Notice to Deviate from Zero |
| NTBi Minutes | Notice to Deliver Bids |
| NTOi Minutes | Notice to Deliver Offers |
| p | BSC Party |
| PARd | Price Average Reference Volume |
| PCLp MW | Purchase Credit Limit |
| PBnij £/MWh | Bid Price |
| POnij £/MWh | Offer Price |
| qAkij(t)MW | Acceptance Volume |
| qAkit MW | Point Acceptance Volume |
| qABknij(t) MW | Accepted Bid Volume |
| qABOknij(t) MW | Accepted Bid-Offer Volume |
| qAOknij(t)MW | Accepted Offer Volume |
| qBOnijt MW | Bid-Offer Volume |
| fqBOnijt MW | Point Bid-Offer Volume |
| QABknij MWh | Period Accepted Bid Volume |
| QAOknij MWh | Period Accepted Offer Volume |
| QABnij MWh | Period BM Unit Total Accepted Bid Volume |
| QABCaj MWh | Account Bilateral Contract Volume |
| QABOaj MWh | Account Period Bid-Offer Volume |
| QACEaj MWh | Account Credited Energy Volume |
| QAEIaj MWh | Account Energy Imbalance Volume |
| QBSABmj | Balancing Services Adjustment Buy Volume |
| QBSASmj | Balancing Services Adjustment Sell Volume |
| QBOij MWh | Period BM Unit Bid-Offer Volume |
| QCEaij MWh | Credited Energy Volume |
| QFPNij(t) MW | Quiescent FPN |
| fQFPNijt MW | Point Quiescent FPN |
| QIIij MWh | Period Information Imbalance Volume |
| QMij MWh | BM Unit Metered Volume |
| QMEij MWh | Period Expected Metered Volume |
| QNDBij MWh | Period BM Unit Non-Delivered Bid Volume |
| QNDBnij MWh | Bid Non-Delivery Volume |
| QNDOij MWh | Period BM Unit Non-Delivered Offer Volume |
| QNDOnij MWh | Offer Non-Delivery Volume |
| QSBwj | System Buy Action |
| QSSwj | System Sell Action |
| RCRCaj £ | Residual Cashflow Reallocation Cashflow |
| RCRPaj No Units | Residual Cashflow Reallocation Proportion |
| RCC £ | Required Credit Cover |
| gRDEi MW | Run-Down Elbow(s) |
| gRDRi MW/Minute | Run-Down Rate(s) |
| RPARd | Replacement Price Average Reference Volume |
| RQNDBuij MWh | Remaining Period BM Unit Non-Delivered Bid Volume |
| RQNDOuij MWh | Remaining Period BM Unit Non-Delivered Offer Volume |
| gRUEi MW | Run-Up Elbow(s) |
| gRURi MW/Minute | Run-Up Rate(s) |
| SAPwj | System Action Price |
| SBPj £/MWh | System Buy Price |
| SECALFi | Supplier Export Credit Assessment Load Factor |
| SELi MW | Stable Export Limit |
| SCLp MW | Sale Credit Limit |
| SILi MW | Stable Import Limit |
| SSPj £/MWh | System Sell Price |
| TCBMj £ | Total System BM Cashflow |
| TCEIj £ | Total System Energy Imbalance Cashflow |
| TCIIj £/MWh | Total System Information Imbalance Charge |
| TCNDj £/MWh | Total System Non-Delivery Charge |
| Tkit | Bid-Offer Acceptance Time |
| TLMij No Units | Transmission Loss Multiplier |
| TQABj MWh | System Total Accepted Bid Volume |
| TQAOj MWh | System Total Accepted Offer Volume |
| TRCj £ | Total System Residual Cashflow |
| u | Non-Delivery Order Number |
| w | System Action |
| z | Energy Contract Volume Notification Agent |

G-2 Glossary of terms:

**Acceptance Volume (qAkij(t)) MW**

The Acceptance Volume (qAkij(t)) is the absolute level of operation at time t implied as a result of Bid-Offer Acceptance k, for BM Unit i in Settlement Period j.

**Accepted Bid Volume (qABknij(t)) MW**

The Accepted Bid Volume (qABknij (t)) is the volume of Bid n accepted as a result of Bid-Offer Acceptance k from BM Unit i at spot times t within Settlement Period j.

**Accepted Bid-Offer Volume (qABOknij(t)) MW**

The Accepted Bid-Offer Volume (qABOknij (t)) is the volume of Bid or Offer from Bid-Offer Pair n accepted as a result of Bid-Offer Acceptance k in Settlement Period j from BM Unit i.

**Accepted Offer Volume (qAOknij(t)) MW**

The Accepted Offer Volume (qAOknij (t)) is the volume of Offer n accepted as a result of Bid-Offer Acceptance k from BM Unit i at spot times t within Settlement Period j.

**Account Bilateral Contract Volume (QABCaj) MWh**

The Account Bilateral Contract Volume (QABCaj) is the sum of all notified (and accepted) Bilateral Total Energy Contract Volumes for Energy Account a in Settlement Period j

**Account Credited Energy Volume (QACEaj) MWh**

The Account Credited Energy Volume (QACEaj) is the aggregate of the BM Unit Metered Volumes allocated to Energy Account a in Settlement Period j.

**Account Energy Imbalance Cashflow (CAEIaj) £**

The Account Energy Imbalance Cashflow (CAEIaj) is the total cashflow resulting from the Energy Imbalance of Energy Account a in Settlement Period j.

**Account Energy Imbalance Volume (QAEIaj) MWh**

The Account Energy Imbalance Volume (QAEIaj) is the volume of Energy Imbalance for Energy Account a in Settlement Period j.

**Account Period Bid-Offer Volume (QABOaj) MWh**

The Account Period Bid-Offer Volume (QABOaj) is the sum of the volume of all accepted Bids and Offers from all BM Units for which Energy Account a is the Lead Energy Account in Settlement Period j.

**Accreditation**

Accreditation has been replaced by Qualification, please refer to Qualification in this glossary. This term is retained to maintain compatibility with the IDD flow definitions.

Advice Note and Statement

Statements produced by the FAA advising BSC Parties of their debits/credits.

**Aggregation**

The process used by the CDCA to produce aggregated energy volumes for Settlement.

**Aggregation Rules**

The rules governing the aggregation of Metering System data to produce total aggregated volumes for transfer to Settlement. An Aggregation Rule may be defined at Metering System, Boundary Point BM Unit and Trading Unit levels.

**Ancillary Services**

Services required to ensure the stable and secure operation of the Transmission Network. These services include the provision of frequency, response, reserve, reactive power and black start.

**Applicable Dispensation**

A Dispensation or a Generic Dispensation which has been granted by the Customer and is applicable to a particular Metering Equipment.

**Auditor**

The organisation appointed by the Customer to provide assurance on the operation of Settlement and correctness of the allocation of Credits and Debits.

**Authentication**

A process performed by the CRA to determine the validity of the originator or recipient of data.

**Balancing and Settlement Code**

The rules, systems and processes underpinning the new balancing and settlement arrangements.

**Balancing and Settlement Code Service Agent**

An Agent that acts on behalf of the Balancing and Settlement Code Company to operate Balancing and Settlement Code processes.

**Balancing and Settlement Code Company Costs**

The costs associated with all of the agency functions that are operated on behalf of the Balancing and Settlement Code Company, and of other Balancing and Settlement Code Company activities.

**Balancing and Settlement Code Start Date**

The first Settlement Day for which electricity over the Total System is settled under the terms of the Balancing and Settlement Code.

**Balancing and Settlement Code Panel**

A panel to supervise proposed modifications to the BSC.

**Balancing Mechanism Report**

A report produced by the Settlement Administration Agent after each Settlement Day, detailing activities on the Balancing Mechanism and estimated imbalance Prices.

**Balancing Mechanism Reporting Agent**

A Balancing and Settlement Code Company Service Agent responsible for relaying to Parties information about the Balancing Mechanism.

**Balancing Mechanism Reporting Service**

The service carried out by the Balancing Mechanism Reporting Agent in capturing system related status information and Balancing Mechanism data and publishing this to BSC Parties and the public in order to present a near to real-time representation of the electricity markets and the Balancing Mechanism.

**Balancing Mechanism Reporting System**

A system used by the Balancing Mechanism Reporting Agent to provide information about the Balancing Mechanism.

**Balancing Mechanism Window Period**

The Balancing Mechanism Window for any time, t, is a time period with a duration of the Gate Closure Period that starts at the end of the half hour period for which Gate Closure has most recently passed.

**Bid**

Refers to a submission indicating a willingness to decrease the volume of MW delivered in the Balancing Mechanism through a decrease in generation or an increase in demand.

**Bid Non-Delivery Volume (QNDBnij) MWh**

The Bid Non-Delivery Volume (QNDBnij) is the volume of non-delivery apportioned to Bid n from BM Unit i in Settlement Period j.

**Bid Number (n)**

A number identifying a particular Bid.

**Bid Price (PBnij) £/MWh**

The Bid Price (PBnij) is the Price at which a BSC Party is willing to buy an additional MWh of Bid n from BM Unit i in Settlement Period j.

**Bid-Offer Acceptance**

A Bid-Offer Acceptance is the purchase and/or sale of Offers and/or Bids by the System Operator in its operation of the Balancing Mechanism.

**Bid-Offer Acceptance Data**

Bid-Offer Acceptance Data is that data which is sent by the System Operator to a BSC Party in order to accept a Bid and/or Offer.

**Bid-Offer Acceptance Number (k)**

The Bid-Offer Acceptance Number (k) is a number identifying a particular set of Bid-Offer Acceptance Data.

**Bid-Offer Acceptance Time (Tkit)**

The Bid-Offer Acceptance Time (Tkit) is the time at which the System Operator issues Bid-Offer Acceptance k.

**Bid-Offer Data**

The Bid-Offer Data comprises is made up of a series of Bid-Offer Pairs and, if appropriate, associated information that links Bids and Offers from a particular BM Unit to those from other BM Units.

**Bid-Offer Lower Range (BOLRnij(t)) MW**

The Bid-Offer Lower Range (BOLRnij(t)) is calculated for Bid-Offer Pairs with negative Bid-Offer Pair Numbers. It is used to determine the operating range (in absolute MW) below FPN in which a particular Bid-Offer Pair applies.

**Bid-Offer Pair**

A Bid-Offer Pair comprises:

a set of Point Bid-Offer Volumes fqBOnijt expressed in MW for spot times t falling within Settlement Period j.

an associated Offer Price POnij and Bid Price PBnij expressed in £/MWh.

an associated Bid-Offer Pair Number n. This is also set to be the Bid-Number of the Bid and the Offer Number of the Offer.

**Bid-Offer Pair Number (n)**

A number used to identify a particular Bid-Offer Pair. Values of n are negative for Bid-Offer Pairs that cover operating levels below FPN and positive for those that cover operating levels above FPN.

**Bid-Offer Upper Range (BOURnij(t)) MW**

The Bid-Offer Upper Range (BOURnij(t)) is calculated for Bid-Offer Pairs with positive Bid-Offer Pair Numbers. It is used to determine the operating range (in absolute MW) below FPN in which a particular Bid-Offer Pair applies.

**Bid-Offer Volume (qBOnij(t)) MW**

The Bid-Offer Volume (qBOnij(t)) is the volume available (relative to FPN) from Bid-Offer Pair n, in Settlement Period j for BM Unit i. Whilst it is, in theory a function of time and can vary across the Settlement Period, it is initially a fixed value.

**Black Start**

The procedure necessary for a recovery from a Total Shutdown or Partial Shutdown of the Total System.

**Black Start Capability**

The ability for at least one of a Power Station of Centrally Despatched Generating Units to start up for shutdown and to energise a part of the transmission system without an external electric power supply.

**BM Unit**

A BM Unit is a point of entry, or exit, to the transmission system where a Final Physical Notification will be required from a Party. For Demand this will normally be a Grid Supply Point Group except where there is a Trading Unit directly connected to the Transmission System. For generation it will normally be a Boundary Point for a single genset.

**BM Unit Credit Assessment Export Capability (BMCAECi) MW**

A value maintained for credit assessment purposes reflecting the transmission access export rights of the BM Unit, GCi, corrected by the Credit Assessment Load Factor.

**Working Day BM Unit Credit Assessment Export Capability (WDBMCAECi) MW**

A value maintained for credit assessment purposes reflecting the transmission access export rights of the BM Unit, GCi, corrected by the Credit Assessment Load Factor, for Working Days.

**Non-Working Day BM Unit Credit Assessment Export Capability (NWDBMCAECi) MW**

A value maintained for credit assessment purposes reflecting the transmission access export rights of the BM Unit, GCi, corrected by the Credit Assessment Load Factor, for non-Working Days.

**BM Unit Credit Assessment Import Capability (BMCAICi) MW**

A value maintained for credit assessment purposes reflecting the transmission access import rights of the BM Unit, DCi, corrected by the Credit Assessment Load Factor.

**Working Day BM Unit Credit Assessment Import Capability (WDBMCAICi) MW**

A value maintained for credit assessment purposes reflecting the transmission access import rights of the BM Unit, DCi, corrected by the Credit Assessment Load Factor, for Working Days.

**Non-Working Day BM Unit Credit Assessment Import Capability (NWDBMCAICi) MW**

A value maintained for credit assessment purposes reflecting the transmission access import rights of the BM Unit, DCi, corrected by the Credit Assessment Load Factor, for non-Working Days.

**BM Unit Identifier Number (i)**

A unique identifier for each BM Unit, generally denoted by (i).

**BM Unit Lead Party**

The BM Unit Lead Party is responsible for submitting all Balancing Mechanism data for a specified BM Unit.

**BM Unit Metered Volume (QMij) MWh**

The BM Unit Metered Volume (QMij) is the metered generation or demand associated with BM Unit i in Settlement Period j.

**BM Unit Period Non-Delivery Charge (CNDij) £**

The BM Unit Period Non-Delivery Charge (CNDij) is the total non-delivery charge associated with the non-deliver of Bids or Offers for BM Unit i in Settlement Period j.

**BM Unit Subsidiary Party**

A number of parties (Lead and Subsidiary) may split the imbalance liabilities associated with a BM Unit. The BM Unit Subsidiary Party/Parties take a percentage of the imbalance liabilities but is/are not responsible for submitting Balancing Mechanism data for that BM Unit.

**Boundary Point**

A Meter Point is a single physical point of entry or exit to the Total System.

**British Grid Systems Agreement**

An agreement governing technical aspects of the interconnection between the transmission networks of the Transmission Company’s , Scottish Power and Scottish and Southern Energy.

**BSC Panel Ruling**

A ruling made by the Balancing and Settlement Code Panel in respect of a BSC Party in a Credit Default position.

**Category 1 Revisit**

A grade of Revisited Site categorised according to the degree of non-compliance for charging purposes.

**Category 2 Revisit**

A grade of Revisited Site categorised according to the degree of non-compliance for charging purposes.

**Central Data Collection Agent**

A Balancing and Settlement Code Service Agent responsible for the collection of metered data from Boundary Points that are registered under the Central Registration Agent.

**Central Registration Agent**

The Central Registration Agent will register Balancing and Settlement Code Parties, BM Units, Trading Units, and Boundary Points other than meters registered in Supplier Meter Registration systems.

**Certificate of Competence**

The certificate of competence required to be held by individual Technical Assurance Agent’s staff in order to comply with safety rules.

**Certification**

Certification has been replaced by Qualification, please refer to Qualification in this glossary. This term is retained to maintain compatibility with the IDD flow definitions.

**Channel or Meter Number**

A number allocated to a data stream from Metering Equipment.

A number allocated to an individual Meter within a Metering Equipment at an installation where there is more than one Meter installed.

**Circuit Identifier**

A name or number or combination of alpha-numeric characters which permit the unique identification of a circuit at a site.

**Code of Practice (COP)**

Codes of Practice issued by the Customer relating to Metering Equipment. Each Code of Practice specifies the set of measured quantities and accuracies that are required to be provided by the Metering System.

**Commissioning Information**

The programme performed on all new Metering Equipment, which is to provide metering data for Settlement, as defined in the relevant Code(s) of Practice.

**Confirmation Notice**

A notice sent to each BSC Party setting out (amongst other things) the total amount received into the FAA Clearing Account.

**Contact Point**

The single point of contact provided by the Technical Assurance Agent.

**Credit Assessment Export Capability**

A value maintained for credit assessment purposes reflecting the transmission access export rights of the BM Unit, GCi, corrected by the Credit Assessment Load Factor.

**Credit Assessment Import Capability (BMCAICi)**

A value maintained for credit assessment purposes reflecting the transmission access import rights of the BM Unit, DCi, corrected by the Credit Assessment Load Factor.

**Working Day Credit Assessment Load Factor (WDCALFi), Non-Working Day Credit Assessment Load Factor (NWDCALFi) and Supplier Export Credit Assessment Load Factor (SECALFi)**

An administered load factor for a BM Unit under the control of the Balancing and Settlement Code Panel used to derive credit cover requirements from transmission access rights.

**Credit Assessment Purchase Price CAPP (£/MWh)**

An administered Price used to value the liabilities of a BSC Party in respect of a shortfall of energy or purchase from the system, for the purposes of calculating credit cover requirements. CAPP will be positive.

**Credit Assessment Sale Price CASP (£/MWh)**

An administered Price used to value the liabilities of a BSC Party in respect of an excess of energy or sale from the system, for the purposes of calculating credit cover requirements. CASP will be zero or negative.

**Credit Cover**

Credit Cover is required from all BSC Parties to a level consistent with an assessment of their possible liabilities to Balancing and Settlement Code Settlement.

**Credit Cover Contract Duration (CCCD)**

The number of days of potential exposure for which credit cover must be provided. CCCD will be set to 28 reflecting the lag between the Settlement Day and the Initial Payment Date.

**Credit Cover Physical Duration (CCPD)**

The number of days of potential exposure for which credit cover must be provided. CCCP will be set to 28 plus the number of days required to disconnect or transfer customers following a party’s default.

**Credit Default**

Credit Default arises where a BSC Party fails to provide the Credit Cover Required or, where the Credit Cover provided is not sufficient to cover any outstanding debt.

**Credit Policy**

The Credit Policy determined by the Customer that is required from all BSC Parties to a level that is consistent with an assessment of their possible liabilities.

**Credited Energy Percentage (CEPaij) %**

The Credited Energy Percentage (CEPaij) is the percentage allocation of the metered volume from BM Unit i (adjusted for Balancing Mechanism action) to be allocated to Energy Account a in Settlement Period j.

**Credited Energy Percentage Authorisation**

A Credited Energy Percentage Authorisation is required to permit the submission of Credited Energy Percentages by a Credited Energy Percentage Notification Agent, and for the validation of these data.

**Credited Energy Percentage Notification**

The notification of Credited Energy Percentages by a CEPNA to an ECVAA.

**Credited Energy Percentage Notification Agent**

Credited Energy Percentage Notification Agents will submit Credited Energy Percentages to the Energy Contract Volume Aggregation Agent, on behalf of the BM Unit Lead and Subsidiary Parties.

**Credited Energy Volume (QCEaij) MWh**

The Credited Energy Volume (QCEaij) is the allocation of the metered volume from BM Unit i (adjusted for Balancing Mechanism action) to be allocated to Energy Account a in Settlement Period j.

**Current Transformer Ratio**

The nominal turns ratio between the primary and secondary windings of a current transformer. (e.g. a 300 ampere primary and 5 ampere secondary windings would be shown as a ratio of 300/5).

**Data Collector ID**

The unique identifier for a Data Collector.

**Data Collector Instation**

Electronic hardware and software or computer systems used to collect online data from remote Metering Equipment. Usually located at the Data Collectors offices.

**Data Collector Outstation Type**

Equipment which receives and stores data from a Meter(s) for the purpose of transfer of that metering data to the Central Data Collection Agent and which may perform some processing before such transfer. This equipment may be in one or more separate units or may be integral with the Meter.

**Deemed Bid-Offer Flag**

The Deemed Bid-Offer Flag is a flag that is activated if the Bid-Offer Acceptance issued by the System Operator is accepting Deemed Bids and/or Offers.

**Deemed Bid**

A Bid that utilises Default Data and which may only be accepted by the System Operator when relevant freely submitted Bids and/or Offers have been exhausted.

**Deemed Data**

Deemed Data includes Deemed Bids and Deemed Offers and associated Prices.

**Deemed Offer**

An Offer that utilises Default Data and which may only be accepted by the System Operator when relevant freely submitted Bids and/or Offers have been exhausted.

**Default Data**

Data items utilised in settlements, or in selecting Bid-Offer Acceptances where the data items have not been submitted, or have been submitted but rejected.

**Demand Capacity (MW)**

The maximum demand of MW and MVAr of electricity

**Direct Connected Consumer Demand**

Demand that is electrically connected to the distribution system of a Public Electricity Supplier and is not directly connected to the Transmission Company’s transmission system

**Dispute**

An objection raised by a BSC Party, the System Operator or by BSCCo Ltd if they object to the results of a Settlement when they believe that the calculation has been undertaken using the wrong data or the calculation does not follow the rules. The Settlement Administration Agent may also raise a dispute on behalf of BSC Parties if errors in calculations or data are detected or suspected.

**Dispute Run**

A re-run of the settlement process where a dispute has been resolved between parties or the Customer has decided the outcome.

**Distribution**

The distribution of electricity over the system of a Public Electricity Supplier.

**Distribution Networks**

The system consisting (wholly or mainly) of electric lines owned or operated by a Public Electricity Supplier (PES)and used for the distribution of electricity from Grid Supply Points or Generating Units or other entry points to the point of delivery to users, and operated by such Public Electricity Supplier excluding any part of the Transmission Company’s Transmission System;

**Distribution System Operator**

The Public Electricity Suppliers, as operators of a distribution network.

**Dynamic Data**

Dynamic Data is a collective term for the following parameters:

Run-Up Rate(s) gRURI;

Run-Up Elbow(s) gRUEI;

Run-Down Rate(s) gRDRI;

Run-Down Elbow(s) gRDEI;

Maximum Export Limit MELj(t);

Maximum Import Limit MILj(t);

Notice to Deviate from Zero NDZI;

Notice to Deliver Offers NTOI;

Notice to Deliver Bids NTBi ;

Minimum Zero Time MZTI;

Minimum Non-Zero Time MNZTI;

Maximum Delivery Volume MDVI;

Maximum Delivery Period MDPI;

Stable Export Limit SELI;

Stable Import Limit SILI.

**Electronic Registration System**

The present system which registers Suppliers’ Metering Systems above 100kW.

**Embedded Demand**

Demand that is electrically connected to the distribution system of a Public Electricity Supplier and is not directly connected to the Transmission Company’s transmission system.

**Embedded Generation**

A generator that is electrically connected to the distribution system of a Public Electricity Supplier and is not directly connected to Transmission Company’s transmission system.

**Energy Account**

BSC Parties will in general have two Energy Accounts, one for their Production Activity and one for their Consumption Activity. Each Energy Account will belong to a single BSC Party.

**Energy Account Number a**

Each Energy Account will have a unique Energy Account Number, generally denoted by the letter a or b.

**Energy Contract Purchase Credit Limit ECPCL (MW)**

For each BSC Party, purchase Energy Contract Volumes notified for Initial Settlement will be capped by its Energy Contract Purchase Credit Limit, applied over the daily average of gross Energy Contract Volumes.

**Energy Contract Sales Credit Limit ECSCL (MW)**

For each BSC Party, sales Energy Contract Volumes notified for Initial Settlement will be capped by its Energy Contract Sale Credit Limit, applied over the daily average of gross Energy Contract Volumes.

**Energy Contract Volume**

Energy Contract Volumes are data submitted to settlement to allow BSC Parties to offset imbalances and reflect bilateral trading of energy.

**Energy Contract Volume Aggregation Agent**

The Energy Contract Volume Aggregation Agent will receive, validate and aggregate notifications of Energy Contract Volumes, and provide the Settlement Administration Agent with the net aggregate position of each BSC Party for each Settlement Period.

**Energy Contract Volume Authorisation**

An Energy Contract Volume Authorisation is required to permit the submission of Energy Contract Volumes by an Energy Contract Volume Notification Agent, and for the validation of these data.

**Energy Contract Volume Day Data**

The Energy Contract Volumes in an Energy Contract Volume Day Notification.

**Energy Contract Volume Day Notification**

An Energy Contract Volume Day Notification will permit the submission in a single file of Energy Contract Volumes for each Settlement Period of a Settlement Day.

**Energy Contract Volume Evergreen Flag**

An element of an Energy Contract Volume Day Notification permitting the submission of a pattern Energy Contract Volumes that will be repeated for every Settlement Day until replaced by a new notification.

**Energy Contract Volume Notification**

An Energy Contract Volume Day Notification or an Energy Contract Volume Period Notification.

**Energy Contract Volume Notification Agent**

Energy Contract Volume Notification Agents will submit Energy Contract Volumes to the Energy Contract Volume Aggregation Agent, on behalf of the Energy Contract Volume Parties.

**Energy Contract Volume Notification Agent Identifier**

A unique identifier for each Energy Contract Volume Notification Agent.

**Energy Contract Volume Party**

The Energy Contract Volume Parties are the two BSC Parties which are the counter parties to an Energy Contract Volume.

**Energy Contract Volume Period Data**

The Energy Contract Volume in an Energy Contract Volume Period Notification.

**Energy Contract Volume Period Notification**

An Energy Contract Volume Period Notification will permit the submission of Energy Contract Volumes for a single Settlement Period.

**Energy Imbalance Prices**

The System Sell Price and the System Buy Price.

**Export Active Energy**

The electrical energy produced, flowing or supplied by an electric circuit during a time interval, and being the integral with respect to time of the instantaneous power, measured in units of watt-hours. In general terms Export Active Energy is deemed to flow towards the transmission system.

**Export Reactive Energy**

The product of voltage and current and the sine of the phase angle between them measured in units of kV volt-amperes reactive and standard multiples thereof as determined by the relevant Code of Practice.

**Externally Interconnected System Operator**

For each external Interconnector with the Total System, the system operator of the interconnected system will be known as an Externally Interconnected System Operator.

**Final Physical Notification (FPNij(t)) MW**

The Final Physical Notification for BM Unit is the level of generation or demand (as the case may be) that the BSC Party expects to generate or consume from BM Unit i, in the absence of any Balancing Mechanism Acceptances from the System Operator. The value of FPNij(t) is calculated for spot times t in Settlement Period by linear interpolation from the values of Point FPN.

**Final Physical Notification Data**

Final Physical Notification Data incorporates Point FPN Data and Point Quiescent FPN Data.

**Funds Administration Agent**

The Funds Administration Agent will effect the payments resulting from Settlement, maintain financial and tax documentation, and manage credit and default arrangements.

**Gate Closure**

Gate Closure for a particular Settlement Period is the spot time one Gate Closure Period in advance of the spot time at the start of that Settlement Period.

**Gate Closure Period (Time)**

The Gate Closure Period is the length of time between Gate Closure and the spot time at the start of the associated Settlement Period. It is set at 4 hours.

**Generation**

The production of electricity.

**Generation Capacity (MW)**

The normal full load capacity of a generating unit.

**Generator**

A person who generates electricity under licence or exemption under the Electricity Act 1989.

**Genset**

Plant or apparatus for the production of electricity.

**Good Industry Practice**

The exercise of that degree of skill, diligence, prudence and foresight, which would reasonably and ordinarily be expected from a skilled and experienced operator engaged in the provision of services similar to the Services.

**Grid Entry Point**

The point at which a Power Station which is not embedded connects to the Transmission Company’s Transmission System.

**Grid Operator**

Operates the transmission system with the objective of providing a reliable supply and maintaining voltage and frequency within the standards laid down in the transmission licence. Using the generator’s offer data the GO schedules and despatches generating sets (gensets) to meet demand whilst attempting to ensure the security and integrity of the transmission system.

**Grid Code**

A code of that name established pursuant to the Transmission Licence.

**Grid Supply Point**

Any point where electricity is delivered from the transmission system to a distribution system.

**Grid Supply Point Group**

Several Grid Supply Points, usually within the geographical area of a Public Electricity Supplier, which are grouped together for Settlement purposes.

**GSP Groups**

A distinct electrical system, consisting of all or part of a distribution system (owned and operated by a Distributor) that is supplied by one or more GSPs for which total supply into the GSP Group can be determined for each half hour.

**GSP Group Take**

The total demand metered at Grid Supply Points net of 100k W supplies handled by the SMRA, Station Demand, Interconnector Demand and inter GSP Group metering.

**Half Hourly Meter**

A meter which provides measurements on a half hourly basis.

**Half-Hour Data Aggregation Agent (HHDAA)**

A party which aggregates data from half-hourly meters, under the Stage 2 Settlement process.

**Half-Hour Data Collection Agent (HHDCA)**

A party which collects data from half-hourly meters under the Stage 2 Settlement process.

**Hand Held Unit (HHU)**

Also known as an Interrogation Unit or Local Interrogation Unit LIU, or a portable computer, which can enter Metering Equipment parameters and extract information from the Metering Equipment and store this for later retrieval.

**Host Public Electricity Supplier Distribution Business**

See PES Distribution Business.

**Import Active Energy**

The electrical energy produced, flowing or supplied by an electric circuit during a time interval, and being the integral with respect to time of the instantaneous power, measured in units of watt-hours. In general terms Export Active Energy is deemed to flow away from the transmission system.

**Import Reactive Energy**

The product of voltage and current and the sine of the phase angle between them measured in units of kV volt-amperes reactive and standard multiples thereof as determined by the relevant Code of Practice.

**Information Imbalance Charge (CIIij) £**

The Information Imbalance Charge (CIIij) is the charge applicable to the associated Lead Energy Account as a result of the Information Imbalance from BM Unit i in Settlement Period j.

**Information Imbalance Price (IIPj) £/MWh**

The Information Imbalance Price (IIPj) is the Price used to settle Information Imbalances. It is initially set to zero.

**Initial Payment Date**

The date at which the payments in respect of Initial Settlement for a Settlement Day are made, on average 28 days after the Settlement Day.

**Initial Physical Notification (IPN)**

The physical notification made to the System Operator on the day ahead probably at 15:00, which can be revised until Gate Closure (four hours before delivery) when it becomes a FPN.

**Initial Settlement**

The Initial Settlement Run will take place about 24 days after the Settlement Day, for payments to be effected about 28 days after the Settlement Day.

**Initial Settlement Report**

A report of data used in and created by Initial Settlement.

**Initial Settlement Timescales**

The timescales for the submission of data to the SAA for Initial Settlement purposes.

**Inspection Schedule**

The TAA Site Inspection Schedule.

**Instation Universal Co-ordinated Time**

The international time standard used by an Instation.

**Interconnector**

An Interconnector is an apparatus for the transmission of electricity to and from the Transmission Company’s transmission system or a Public Electricity supplier distribution system into or out of an external system.

**Interconnector Administrator**

The Interconnector Administrator administers Interconnector capacity entitlements and provides information for Settlement.

**Interconnector Emergency Support**

The procedures for system-to-system assistance across Interconnectors.

**Interconnector Emergency Support Offer Price (IESOPij) £/MWh**

A Price submitted by an Interconnector User and used to settle energy flows arising from Interconnector Emergency Support.

**Interconnector Error Account**

An Energy Account associated with an Interconnector Error Administrator.

**Interconnector Error Account BM Unit**

A BM Unit allocated to the relevant Interconnector Error Administrator in respect of each Interconnector.

**Interconnector Error Administrator**

The Interconnector Error Administrator is a BSC Party responsible for any difference between the Interconnector metered flow and the aggregated volumes of Interconnector Users.

**Interconnector User**

Any party that is able to notify flows across an Interconnector and have them deemed delivered is an Interconnector User for that Interconnector. Interconnector Users are required to be parties to the England & Wales Balancing and Settlement Code and to the arrangements governing Interconnector access.

**Interim Initial Settlement**

The Interim Initial Settlement Run will take place at about 4 days after the Settlement Day.

**Keys**

A system(s) or process(s) that enables the BSC Party or BSC Service Agent to authenticate the originator or recipient of data.

**Kilowatt (kW)**

1000 watt.

**Kilowatt Hour (kWh)**

The energy delivered by 1kW over 1 hour.

**Lead Energy Account**

The Lead Energy Account is the Energy Account of the Registrant of the Boundary Point associated with a particular BM Unit.

**Lead Party**

The BSC Party that is responsible for the Lead Energy Account of a particular BM Unit and who registers the Boundary Point(s) associated with a particular BM Unit.

**Licensed Distribution System Operator (LDSO)**

Generic term for any Party which operates an electricity distribution network.

**Line Loss Class**

A set of Metering Systems that are assigned the same Line Loss Factor.

**Line Loss Factor (LLF)**

A multiplier applied to correct metered volumes at embedded Boundary Points to a Grid Supply Point to account for electrical losses in the distribution system.

**Line Loss Factor Class**

A class of Line Loss which applies to a group of Metering Systems where a group may be one or more Metering Systems.

**Market Domain Data**

Data provided to all persons involved in settlements in accordance with the Balancing and Settlement Code.

**Maximum Delivery Period (MDPi(t)) Minutes**

At any time t, the Maximum Delivery Period (MDPi(t)) is the time period over which the Maximum Delivery Volume restriction applies for BM Unit i.

**Maximum Delivery Volume (MDVi(t)) MW**

At any time t, the Maximum Delivery Volume (MDVi(t)) is the maximum number of MWh of Offer (or Bid if negative), that a particular BM Unit i may deliver on a cumulative basis within the associated Maximum Delivery Period.

**Maximum Export Limit (MEL i(t)) MW**

The Maximum Export Limit (MEL i(t)) is the maximum power export that a BM Unit is capable of at time t.

**Maximum Import Limit (MIL ij(t)) MW**

The Maximum Import Limit (MILi(t)) is the maximum power export that a BM Unit is capable of at time t.

**Megawatt (MW)**

1,000 kW.

**Meter**

A device for measuring active and/or reactive energy.

**Meter Advance Reconciliation**

The process of comparing physical meter register advances with electronically gathered half hourly consumption data over a defined period of time

**Meter Commissioning Date**

The date on which any Metering System or Metering Equipment is commissioned in accordance with the relevant Code of Practice.

**Meter Constant**

A multiplier or fraction, which is applied to the measurement quantities so as to obtain the real value of Energy measured.

**Meter Manufacturer**

The manufacturer of the Metering Equipment, usually recorded for the Meter only. The whole Metering Equipment may comprise components from a range of manufacturers.

**Meter Operator Agent (MOA)**

An organisation accredited to install, commission and maintain the physical meters and communications equipment compliant with Codes of Practice that comprises a Metering System.

**Meter Operator Agent Appointment Date**

The date of appointment of a Meter Operator Agent for a particular Metering System.

**Meter Point**

A Meter Point means the point at which a supply to (export) or from (import) a Distribution System is measured.

**Meter Pulse Multiplier**

A constant, multiplier or fraction, which is applied to pulsed outputs to derive an Energy value for each pulse. This value may also be used in conjunction with a Meter Constant.

**Meter Reading Schedule**

A schedule produced by the CDCA that details the timing and frequency of meter readings required for the Meter Advance Reconciliation (MAR) process.

**Meter Serial Number**

The serial number as shown on the nameplate on the front of a Meter.

**Meter Test Certificate**

A certificate recording the accuracy and calibration details of an individual Meter.

**Meter Type**

A Half Hourly or Non-half hourly Meter.

A Manufacturers model or identification markings.

**Metered Volume Fixed Reallocation**

A fixed allocation, specified in MWh, of a BM Unit Metered Volume, which is credited to the Energy Account of a Subsidiary Party from the Energy Account of the Lead party at the relevant BM Unit.

**Metered Volume Percentage Reallocation**

A percentage allocation of a BM Unit Metered Volume after the deduction of any Metered Volume Fixed Reallocations and Period Accepted Bid and Offer Volumes, which is credited to the Energy Account of a Subsidiary Party from the Energy Account of the Lead Party at the relevant BM Unit.

**Metered Volume Reallocation Notification**

A notification submitted by the Metered Volume Reallocation Agent on behalf of BM Unit Lead and Subsidiary Parties and compromising a set of Metered Volume Fixed Reallocations and a set of Metered Volume Percentage Reallocations (note that a Metered Volume Reallocation Agent is synonymous with and replaces the Credited Energy Percentage Notification Agent).

**Metering Code of Practice**

One of the documents of that name currently established pursuant to the Pooling and Settlement Agreement.

**Metering Equipment**

Meters, measurement transformers (voltage, current or combination units), metering protection equipment including alarms, circuitry, associated communications equipment and outstations and wiring, which are part of the Active Energy and/or Reactive Energy measuring and transmitting equipment for Settlement.

**Metering Inside Settlement Timescales**

Half-hourly metering such that data is available for Initial Settlement.

**Metering Outside Settlement Timescales**

Metering such that data is not available for Initial Settlement.

**Metering System**

All or that part of the commissioned Metering Equipment at or relating to a site linked to a single outstation at or relating to that site (including such outstation) which measures a trade in active energy, or as the case may be reactive energy. In this context metering equipment refers to the meters, measurement transformers (voltage, current or combination units), metering protection equipment including alarms, circuitry associated communications equipment and outstations and wiring which are part of the active energy and/or reactive energy measuring and transmitting equipment.

**Minimum Non-Zero Time (MNZTi) Minutes**

At any time t, the Minimum Non-Zero Time (MNZTi) represents the minimum time that BM Unit i can operate at a non-zero level as a result of accepted Balancing Mechanism action.

**Minimum Zero Time (MZTi) Minutes**

At any time t, the Minimum Zero Time (MZTi) is the minimum time that a BM Unit must operate at zero or import, before returning to export; whereas if it is importing, MZT indicates the minimum time that it must operate at zero or export before returning to import, if action by the System Operator places it at such a level.

**Non-Delivered Bid Charge (CNDBnij) £**

The Non-Delivered Bid Charge (CNDBnij) is the charge associated with the non-delivery of Bid n in Settlement Period j from BM Unit i.

**Non-Delivered Offer Charge (CNDOnij) £**

The Non-Delivered Offer Charge CNDOnij is the charge associated with the non-delivery of Offer n in Settlement Period j from BM Unit i.

**Non-Delivery Order Number (u)**

The Non-Delivery Order Number (u) is an index used to rank non-delivered Offers or Bids from a BM Unit in a particular Settlement Period in order to determine the order of allocation the Period BM Unit Non-Delivered Offer Volume, or the Period BM Unit Non-Delivered Bid Volume.

**Non-Half-Hour Data Aggregation Agent (NHHDAA)**

A party which aggregates data from non-half-hourly meters, under the Stage 2 Settlement process.

**Non-Half-Hour Data Collection Agent (NHHDCA)**

A party which collects data from non-half-hourly meters, under the Stage 2 Settlement process.

**Notice to Deliver Bids (NTBi) Minutes**

The Notice to Deliver Bids (NTBi) is a Dynamic Data item that indicates the length of time between the issuing of a Bid-Offer Acceptance and the time when a BM Unit begins to deliver Bid volumes.

**Notice to Deliver Offers (NTOi) Minutes**

The Notice to Deliver Offers (NTOi) is a Dynamic Data item that indicates the length of time between the issuing of a Bid-Offer Acceptance and the time when a BM Unit begins to deliver Offer volumes.

**Notice to Deviate from Zero (NDZi) Minutes**

The Notice to Deviate from Zero (NDZi) expresses the notification time required for a BM Unit to change its consumption or production level from zero.

**Notification Date**

The dates by which the SAA shall deliver the Initial Debits/Credits for each of the Initial Settlement Runs to the FAA.

**Offer**

An Offer refers to a submission indicating a willingness to increase the volume of MW delivered in the Balancing Mechanism through an increase in generation or a decrease in demand.

**Offer Non-Delivery Volume (QNDOnij) MWh**

The Offer Non-Delivery Volume (QNDOnij) is the volume of non-delivery apportioned to Offer n from BM Unit i in Settlement Period j.

**Offer Number (n)**

A number identifying a particular Offer.

**Offer Price (POnij) £/MWh**

The Offer Price (POnij) is the Price at which a BSC Party is willing to sell an additional MWh of Offer n from BM Unit i in Settlement Period j.

**On-Site Procedures**

The procedural documentation and test sheets provided by the Technical Assurance Agent which details the on-site processes to be carried out during a site visit.

**Outstation**

Equipment that receives and stores metering data from meter(s), transfers this data to an instation or hand held device and may perform some processing before transfer. This equipment may be in one or more separate units or may be integral with the meter.

**Over-The-Counter (OTC)**

An OTC contract is one which has been negotiated between two parties directly or through a broker, rather than one where counter-party risk is taken by clearing house, such as a trade on a cleared Power Exchange.

**BSC Party Identifier p**

Each Balancing and Settlement Code Party will be given a unique Balancing and Settlement Code Party Identifier as part of the registration process. The Balancing and Settlement Code Party Identifier is generally denoted p.

**Payment Calendar**

A calendar maintained by the Funds Administration Agent, listing all Initial and Reconciliation Payment Dates for each Settlement Day.

**Payment Date**

Day on which money is transferred after an Initial of Reconciliation Settlement Run.

**Period Accepted Bid Volume (QABknij) MWh**

The Period Accepted Bid Volume (QABknij) is the Settlement Period integrated volume of Bid n, in MWh accepted as a result of Bid-Offer Acceptance k.

**Period Accepted Offer Volume (QAOknij) MWh**

The Period Accepted Offer Volume (QAOknij) is the Settlement Period integrated volume of Offer n, in MWh accepted as a result of Bid-Offer Acceptance k.

**Period Acceptance Bid Cashflow (CABknij) £**

The Period Acceptance Bid Cashflow (CABknij) is the Transmission Loss adjusted cashflow to BM Unit i for Balancing Mechanism action in Settlement Period j, allocated to Bid n, as a result of Bid-Offer Acceptance k.

**Period Acceptance Offer Cashflow (CAOknij) £**

The Period Acceptance Offer Cashflow (CAOknij) is the Transmission Loss adjusted cashflow to BM Unit i for Balancing Mechanism action in Settlement Period j, allocated to Offer n, as a result of Bid-Offer Acceptance k.

**Period BM Unit Total Accepted Bid Volume (QABnij) MWh**

The Period BM Unit Total Accepted Bid Volume (QABnij) is the total volume of Bid n accepted in Settlement Period j from BM Unit i, summed over all Bid-Offer Acceptances.

**Period BM Unit Total Accepted Offer Volume (QAOnij) MWh**

The Period BM Unit Total Accepted Offer Volume (QAOnij) is the total volume of Offer n accepted in Settlement Period j from BM Unit i, summed over all Bid-Offer Acceptances.

**Period BM Unit Bid Cashflow (CBnij) £**

The Period BM Unit Bid Cashflow (CBnij) is the total cashflow resulting from accepted volumes of Bid n from BM Unit i in Settlement Period j.

**Period BM Unit Bid-Offer Volume (QBOij) MWh**

The Period BM Unit Bid-Offer Volume (QBOij) is the volume of accepted Bids and Offers from BM Unit i, summed over Settlement Period j.

**Period BM Unit Cashflow (CBMij) £**

The Period BM Unit Cashflow (CBMij) is the total cashflow resulting from all accepted Bids and Offers from BM Unit i in Settlement Period j.

**Period BM Unit Non-Delivered Bid Volume (QNDBij) MWh**

The Period BM Unit Non-Delivered Bid Volume (QNDBij) is the volume of non-delivered Bids from BM Unit i in Settlement Period j.

**Period BM Unit Non-Delivered Offer Volume (QNDOij) MWh**

The Period BM Unit Non-Delivered Offer Volume (QNDOij) is the volume of non-delivered Offers from BM Unit i in Settlement Period j.

**Period Expected Metered Volume (QMEij) MWh**

The Period Expected Metered Volume (QMEij) is the volume of energy that a particular BM Unit is expected to deliver or consume in Settlement Period j

**Period FPN (FPNij) MWh**

The Period FPN (FPNij) is the integrated MWh of energy implied by integrating the Final Physical Notification for BM Unit i over Settlement Period d.

**Period Information Imbalance Volume (QIIij) MWh**

The Period Information Imbalance Volume (QIIij) is the volume of energy for BM Unit i, in Settlement Period j to which Information Imbalance charges apply.

**Period BM Unit Offer Cashflow (COnij) £**

The Period BM Unit Offer Cashflow (COnij) is the total Cashflow resulting from accepted volumes of Offer n from BM Unit i in Settlement Period j.

**PES Distribution Business**

The Distribution Business of the relevant Public Electricity Supplier.

**Point Acceptance Volume (qAkit) MW**

The Point Acceptance Volume (qAkit) is part of the Bid-Offer Acceptance k. It specifies an absolute MW operating level for BM Unit i at spot time t.

**Point Bid-Offer Volume (fqBOnijt) MW**

The Point Bid-Offer Volume (fqBOnijt) is part of the Bid-Offer Data for Bid-Offer Pair n in Settlement Period j. It specifies the MW of Bid-Offer n available at spot time t for BM Unit i.

Initially only a single value of Point Bid-Offer Volume may be submitted for each Bid-Offer Pair n. If submitted, this value must be for the first spot time of the Settlement Period.

**Point FPN (fFPNijt) MW**

Point FPN (fFPNijt) data is a series of one or more MW spot values submitted for spot times t in Settlement Period j for BM Unit i. It is used to determine the values of Final Physical Notification.

**Point Maximum Export Limit (fMEL it) MW**

The Point Maximum Export Limit (fMEL it) is a positive MW value specifying the maximum export that is possible from BM Unit i at spot time t. It is treated as part of the Dynamic Data.

**Point Maximum Import Limit (fMIL it) MW**

The Point Maximum Import Limit (fMIL it) is a negative MW value specifying the maximum import that is possible from BM Unit i at spot time t. It is treated as part of the Dynamic Data.

**Point Quiescent FPN fQFPNit (MW)**

BSC Traders are permitted to submit values of Point Quiescent FPN, fQFPNit for certain BM Units. A Point Quiescent FPN is a spot value expressing the volume of generation or demand expected to be generated or consumed by an underlying process that forms part of the operation of particular BM Unit at any particular spot time.

**Point Value Identification Number (f)**

The Point Value Identification Number (f) is a number used to differentiate between two values of any point variable submitted for the same spot time.

**Pooling and Settlement Agreement (PSA)**

An agreement which determines the way in which electricity was bought and sold through the Electricity Pool.

**Public Electricity Suppliers (PES)**

Regional Companies that owned and operate the local distribution networks and operated as Suppliers.

**Purchase Credit Limit (PCLp) MW**

For each BSC Trader p, the amount of Energy Contract Volumes (for purchases of energy) and relevant Credited Energy Percentages that can be accepted in respect of its Energy Accounts is limited by its Purchase Credit Limit.

**Qualification**

The process to which BSC Parties and Party Agents will submit prior to becoming Qualified. Please refer to BSCP70 for all Parties and Party Agents except for CVA Meter Operator Agents where reference should additionally be made to BSCP537.

**Qualified BSC Party Agent**

A Qualified BSC Party Agent acts on behalf of BSC Parties, which are responsible for the performance of its function, but is Qualified and Registered under the Balancing and Settlement Code.

**Quiescent FPN (QFPNij(t)) MW**

The Quiescent FPN (QFPNij(t)) is a MW value expressing the volume of generation or demand expected to be generated or consumed by an underlying process that forms part of the operation of particular BM Unit at any particular time.

**Ramp Rate Identification Number (g)**

A number used to differentiate between Run-Up Rates and Run-Down Rates for a particular BM Unit.

**Reactive Power**

An Ancillary Service required to maintain voltages on the Total System within statutory limits.

**Reconciliation Payment Date**

The day at which payments in respect of a Reconciliation Settlement Run are made.

**Reconciliation Settlement Report**

Report of a Reconciliation Settlement Run, produced by the Settlement Administration Agent.

**Reconciliation Settlement Run**

A settlement run to account for data that has become available after Initial Settlement.

**Registration Application**

An application received by the CRA from a BSC Party or BSC Service Agent.

**Remaining Period BM Unit Non-Delivered Bid Volume (RQNDBuij) MWh**

The Remaining Period BM Unit Non-Delivered Bid Volume (RQNDBuij) is the amount of Non-Delivered Bid Volume remaining to be allocated to Bid u.

**Remaining Period BM Unit Non-Delivered Offer Volume (RQNDOuij) MWh**

The Remaining Period BM Unit Non-Delivered Offer Volume (RQNDOuij) is the amount of Non-Delivered Offer Volume remaining to be allocated to Offer u.

**Required Credit Cover RCC £**

For each participant, the Funds Administration Agent will calculate the Required Credit Cover for their Transmission Access Rights and Energy Contract Volume credit limits.

**Reserve**

Generating capacity that can deliver power at very short notice to meet sudden and unexpected increases in demand or loss of power from a generating unit. It is often provided in the form of generating units operating below their declared availability

**Residual Cashflow Reallocation Cashflow (RCRCaj) £**

The Residual Cashflow Reallocation Cashflow (RCRCaj) is the cashflow to Energy Account a in Settlement Period j resulting from the reallocation the Total System Residual Cashflow.

**Residual Cashflow Reallocation Proportion (RCRPaj) No Units**

The Residual Cashflow Reallocation Proportion (RCRPaj) is a fraction expressing the proportion of the Total System Residual Cashflow to be allocated to Energy Account a in Settlement Period j.

**Revisited Sites**

Sites selected for a subsequent inspection following identification of non-compliance.

**Run-Down Elbow(s) (gRDEi) MW**

The Run-Down Elbow (gRDEi) is a MW level used to define a range of operating output within which a particular Run-Down Rate applies. Values apply to BM Unit i. Different values may apply for different MW levels for the same BM Unit at any given time.

**Run-Down Rate(s) (gRDRi) MW/Minute**

The Run-Down Rate(s) (gRDRi) expresses the rate of decrease in active power production or the rate of increase of active power consumption for a particular BM Unit within a particular operating range.

**Run-Up Elbow(s) (gRDEi) MW**

The Run-Up Elbow (gRDEi) is a MW level used to define a range of operating output within which a particular Run-Up Rate applies. Values apply to BM Unit i. Different values may apply for different MW levels for the same BM Unit at any given time.

**Run-Up Rate(s) (gRURi) MW/Minute**

The Run-Up Rate (gRURi) expresses the rate of increase in active power production or the rate of decrease of active power consumption for a particular BM Unit within a particular operating range.

**Sales Credit Limit (SCLp) MW**

For each BSC Trader p, the amount of Energy Contract Volumes (for sales of energy) and relevant Credited Energy Percentages that can be accepted in respect of its Energy Accounts is limited by its Sale Credit Limit.

**Sampled Sites**

Sites selected for inspection by representative sampling from Metering Systems registered with the Central Registration Agency.

**Settlement**

The word Settlement encompasses all aspects of transactions from meter to bank, for all types of imbalances and Balancing Mechanism trades.

**Settlement Administration Agent**

A BSC Service Agent contracted to the BSCCo Ltd to operate the Settlement system.

**Settlement Calendar**

The Calendar created and published by the Settlement Administration Agent on an annual basis to ensure that all Settlement calculations and Runs are performed in a timely manner. The Settlement Calendar shall be derived from and consistent with the Payment Calendar published by the Funds Transfer Agent.

**Settlement Day**

The Settlement Day runs from midnight to midnight (BST during the summer and GMT during the winter).

**Settlement Period j**

A Settlement Period is the lowest possible resolution for the calculation of imbalances, lasting half an hour.

**Settlement Report**

The report issued to BSC Parties by the Settlement Administration Agent which relates to a particular Settlement Run.

**Settlement Run**

Initial and Reconciliation Settlement Runs are performed by the Settlement Administration Agent prior to each Initial or Reconciliation Payment Date, for each Settlement Day.

**Stable Export Limit (SELi) MW**

The Stable Export Limit (SELi) is a positive MW value, expressing the minimum stable export operating level for BM Unit i. It is part of the Dynamic Data.

**Stable Import Limit (SILi) MW**

The Stable Import Limit (SILi) is a negative MW value, expressing the minimum stable import operating level for BM Unit i. It is part of the Dynamic Data

**Standards**

British (BSI) and International (IEC) Standards as applicable to Metering Equipment.

**Subsidiary Energy Account**

A Subsidiary Energy Account is an Energy Account (other than the Lead Energy Account) for which a value of CEP has been submitted for a BM Unit.

**Supplier**

A supplier will be a company that provides electricity supplies to groups of customers based on geography and/or size. The company will be a Party of the Balancing and Settlement Code and will hold a second tier Supply licence unless they are licence exempt.

**Supplier Half-Hourly Data Aggregation Agent**

Supplier Half-Hourly Data Aggregation Agents will aggregate data provided by Supplier Half-Hourly Data Collection Agents and submit them to the Supplier Volume Allocation Agent.

**Supplier Half-Hourly Data Collection Agent**

Supplier Half-Hourly Data Collection Agents will collect data from half-hourly meters registered in the Supplier Meter Registration Agent system.

**Supplier Half-Hourly Meter Operation Agent**

Supplier Half-Hourly Meter Operation Agents will be responsible for installing and maintaining half-hourly meters registered in a SRA system.

**Supplier Meter Administration Agent**

Supplier Meter Administration Agents will provide half-hourly deemed metered volumes for un-metered supplies and submit them to the Supplier Volume Allocation Agent.

**Supplier Meter Registration Agent**

For each Grid Supply Point Group, the Supplier Meter Registration Agent will provide a registration service.

**Supplier Non-Half-Hourly Data Aggregation Agent**

SNHHDAAs will aggregate data provided by a SNHHDCAs and submit them to the Supplier Volume Allocation Agent.

**Supplier Non-Half-Hourly Data Collection Agent**

SNHHDCAs will collect data from non-half-hourly meters registered in a Supplier Meter Registration Agent system.

**Supplier Non-Half-Hourly Meter Operation Agent**

SNHHMOAs will be responsible for installing and maintaining non-half-hourly meters registered in a SRA system.

**Supplier Profile Administration Agent**

The SPAA will maintain profiles for the purposes of determining half-hourly deemed metered amounts, and supply data to the Supplier Volume Allocation Agent.

**Supplier Technical Assurance Agent**

The STAA will ensure compliance with relevant standards for meters registered in a Supplier Meter Registration Agent system. It will also monitor Data Collection Agents.

**Supplier Teleswitching Support Agent**

The STSA will provide the Supplier Volume Allocation Agent with information about switching times for teleswitched non-half-hourly meters.

**Supplier Volume Allocation Agent**

The Supplier Volume Allocation Agent will calculate deemed metered amounts at Grid Supply Point Group level.

**Supply Number**

A Supply number consists of 21 digits that uniquely relate to a single physical metering system used for Settlement purposes. Suppliers use the Supply Number to register their interest in a particular metering system in a PES Supplier Meter Registration System.

**System Buy Price (SBPj) £/MWh**

The System Buy Price (SBPj) is the weighted average of accepted Offers in Settlement Period j.

**System Marginal Price (SMP)**

In the current arrangements, the offer Price of the highest Price station in operation at any time.

**System Operator (SO)**

The entity that fulfils the role of operating the transmission system, including issuing instructions to generators or demand to change its level of output or take, and instructing the provision of Ancillary Services and other measures necessary to maintain a stable and secure system. This role in England and Wales is carried out by The National Grid Electricity Transmission PLC under the terms of its Transmission Licence.

**System Operator BM Charge (CSOBMj) £**

The System Operator BM Charge (CSOBMj) is the amount paid by the System Operator in Settlement Period j.

**System Sell Price (SSPj) £/MWh**

The System Sell Price (SSPj) is the weighted average of accepted Bids in Settlement Period j.

**System Total Accepted Bid Volume (TQABj) MWh**

The System Total Accepted Bid Volume (TQABj) is the sum over all BM Units of all accepted Bids in Settlement Period j.

**System Total Accepted Offer Volume (TQAOj) MWh**

The System Total Accepted Offer Volume (TQAOj) is the sum over all BM Units of all accepted Offers in Settlement Period j.

**TAA Site Inspection Schedule**

A form completed by the Technical Assurance Agent in connection with a site visit.

**TAA Status Report**

The monthly report provided by the Technical Assurance Agent to the Customer.

**Targeted Sites**

Sites selected for inspection by the Technical Assurance Agent following suspicion of non-compliance.

**Technical Assurance Agent**

The Technical Assurance Agent will ensure that metered associated with an Boundary Points registered under the Central Registration Agent conform to the relevant Codes of Practice.

**Technical Circular (TC)**

An authorised change or enhancement to a Code of Practice.

**Total Energy Contract Volume**

(QABCaj) in MWh. The sum of all notified (and accepted) Contract Volumes for Energy Account a in Settlement Period j.

**Total System**

The collection of high voltage wires owned and operated by The Transmission Company’s and the Public Electricity Suppliers in England and Wales, within the geographical boundary of England and Wales.

**Total System BM Cashflow (TCBMj) £**

The Total System BM Cashflow (TCBMj) is the total cashflow summed over all BM Units resulting from the operation of the Balancing Mechanism in Settlement Period j.

**Total System Energy Imbalance Cashflow (TCEIj) £**

The Total System Energy Imbalance Cashflow (TCEIj) is the total cashflow resulting from the Settlement of Energy Imbalances, summed over all Energy Accounts in Settlement Period j.

**Total System Information Imbalance Charge (TCIIj) £/MWh**

The Total System Information Imbalance Charge (TCIIj) is the total charge for information imbalances, summed over all BM Units and Energy Accounts in Settlement Period j.

**Total System Non-Delivery Charge (TCNDj) £/MWh**

The Total System Non-Delivery Charge (TCNDj) is the total charge for non-delivered Bids and Offers summed over all BM Units in Settlement Period j.

**Total System Residual Cashflow (TRCj) £**

The Total System Residual Cashflow (TRCj) is the surplus or deficit of funds remaining to be reallocated after the Settlement of Energy Imbalances, Information Imbalances, the Balancing Mechanism (including non-delivery) and the System Operator BM Charge.

**Trading Unit**

A Trading Unit is a configuration of Boundary Points that are traded at net volume. Constituent Boundary Points must be materially interdependent, or must be linked via a contiguous path of connection assets associated with the parties registered against the Boundary Points.

**Trading Unit Identification Number**

A unique identifier for each Trading Unit.

**Transmission Licence**

Licence required to transmit electricity for the purpose of giving a supply to any premise or enabling a supply to so be given. The Transmission Licence in England and Wales is held by The National Grid Electricity Transmission PLC.

**Transmission Loss Factor (TLFij) No Units**

A factor used in the calculation of Transmission Loss Multipliers.

**Transmission Loss Factor Agent**

The Transmission Loss Factor Agent will derive Adjusted seasonal Zonal TLFs and BM Unit specific TLFs for use in the Settlement Calculations.

**Transmission Loss Multiplier (TLMij)**

The Transmission Loss Multiplier (TLMij) is the factor applied to BM Unit i in Settlement Period j in order to adjust for Transmission Losses.

**Transmission System**

That part of the Total System owned and operated by the holder of the Transmission Licence.

**Unmetered Supply**

A Boundary Point for which the volume of electricity supplied from the Total System is derived without reference to a meter.

**Universal Co-ordinated Time**

The international time standard.

**Universal Time Clock (UTC)**

The Universal Time based on atomic clocks rather than GMT.

**Voltage Transformer Ratio**

The nominal turns ratio between the primary and secondary windings of a voltage transformer. (e.g. a 11,000 volts primary and 110 volts secondary windings would be shown as a ratio of 11,000/110).

**Watt (W)**

A measure of rate of flow of electricity or power flow.

1. A number of the change requests considered in the URS have required changes in terminology. These have not been updated in the Glossary at this issue. [↑](#footnote-ref-2)
2. The Accreditation/Certification details will report Qualification Details, but the name of the Data group is unchanged for IDD compatibility. [↑](#footnote-ref-3)
3. The Accreditation/Certification details will report Qualification Details, but the name of the Data group is unchanged for IDD compatibility. [↑](#footnote-ref-4)
4. A BM Unit must be registered in order to be assigned a BM Unit Identifier. Subsequently, BSCCo Ltd may register the BM Unit as Exempt Export. The two steps to this operation are represented by requirements CRA-I005/CRA-F013 and CRA-I043/CRA-F014 respectively, though logically, they can be considered to be parts of a single registration operation. [↑](#footnote-ref-5)
5. The Accreditation/Certification details will report Qualification Details, but the name of the Data group is unchanged for IDD compatibility. [↑](#footnote-ref-6)
6. For the avoidance of doubt, in the event of a discrepancy between this description and the methodology, the methodology shall prevail. [↑](#footnote-ref-7)
7. If the notification is sent by 15:00, this will be the next Working Day; otherwise it will be the Working Day after that. [↑](#footnote-ref-8)
8. Note that details of the CRA-I012 (Issue CRA Encryption Key) flow have not been included in this diagram, in order to avoid excessive clutter. [↑](#footnote-ref-9)